{"text_format":"2","workbook":"xlsx","n_sheets":9,"sheets":["TD变配电系统 ","DG柴发机房系统","BP备用电源系统","EP机房动力系统","OP室外动力系统","EL电梯系统","LT照明系统","TP租户配电系统","SD强电人防系统"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"TD变配电系统 ","index":0,"n_rows":80,"n_cols":10,"rows_kept":80,"cut":false,"hidden":false,"merged":[[78,0,78,1],[79,0,79,1],[53,0,77,0],[0,0,0,9],[1,0,1,1],[72,1,74,1],[7,1,35,1],[2,0,52,0],[36,1,52,1],[2,1,6,1],[53,1,71,1],[75,1,77,1]]}
["变配电系统"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典说明"," 备注"]
[" 技术参数","整体","电压等级类型","ULevType",null,"Enum","S","D1","1. 高压变配电系统 2. 低压变配电系统 99. 其他"]
[null,null,"用电用户类型","UserType",null,"Enum","S","D1","1. 重要电力用户 2. 工商业电力用户 99. 其他"]
[null,null,"重要电力用户分级","ImportantUserLev",null,"Enum","S","D1","1. 特级 2. 一级 3. 二级 4. 临时性重要电力用户 99. 其他"]
[null,null,"工商业电力用户分级","ICUserLev",null,"Enum","S","D1","1. 重要电力负荷 2. 一级负荷 3. 二级负荷 4. 三级负荷 99. 其他"]
[null,null,"安装地点","InstallLocationType",null,"Enum","M","D1","1. 室外 2. 室内 99. 其他"]
[null,"高压","高压有无母线","HUisBus",null,"Bool","M","E1","0. 无 1. 有"]
[null,null,"高压母线接线类型","HUBusConnectType",null,"Enum","R","D1","1. 单母线 2. 分段单母线 3. 单母线带旁路母线 4. 双母线 99. 其他"]
[null,null,"高压主变压器数量","HUMainTransNum","个","Num","S","A2"]
[null,null,"高压主变压器绕组类型","HUMainTransWindingType",null,"Enum","R","D1","1. 双绕组 2. 三绕组 99. 其他"]
[null,null,"高压变电系统额定进线电压 ","HURatedInU","kV","Num","S","A2"]
[null,null,"高压变电系统额定中压出线电压 ","HURatedOutMediumU","kV","Num","S","A2"]
[null,null,"高压变电系统额定低压出线电压 ","HURatedOutLowU","kV","Num","S","A2"]
[null,null,"高压变电系统设计容量","HUDesignCap","kVA","Num","S","A2"]
[null,null,"高压是否有站内变压器","isHUStationTrans",null,"Bool","M","E1","0. 无 1. 有"]
[null,null,"高压是否有接地变压器","isHUGroundTrans",null,"Bool","M","E1","0. 无 1. 有"]
[null,null,"高压是否有直流屏 ","isHUDCScreen",null,"Bool","M","E1","0. 无 1. 有"]
[null,null,"高压是否为双电源","isHUDualPower",null,"Bool","M","E1","0. 否 1. 是"]
[null,null,"高压双电源运行方式","HUDualPowerOperateType",null,"Enum","M","D1","1. 一用一备 2. 同时运行，互为备用 99. 其他"]
[null,null,"高压站内用电来源","HUStationPowerSource",null,"Enum","R","D1","1. 站内变压器 2. 接地变压器 99. 其他"]
[null,null,"高压出线连接形式","HUOutConnectType ",null,"Enum","R","D1","1. 单回路树干式 2. 双回路树干式 3. 普通环网式 4. 拉手环网式 5. 单回路放射式 6. 双回路放射式 99. 其他"]
[null,null,"高压线路敷设形式","HUWireInstallType",null,"Enum","R","D1","1. 地埋线 2. 架空线 99. 其他"]
[null,null,"高压开关柜连接关系","HUCabConnect",null,"Topology","R","I"]
[null,null,"高压变压器进线柜数量","HUIncomingCabNum","个","Num","R","A2"]
[null,null,"高压隔离柜数量","HUIsolateCabNum","个","Num","R","A2"]
[null,null,"高压断路器柜数量","HUBreakerCabNum","个","Num","R","A2"]
[null,null,"高压计量柜数量","HUMeterCabNum","个","Num","R","A2"]
[null,null,"高压无功补偿柜数量","HUReactiveCompensationCabNum","个","Num","R","A2"]
[null,null,"高压PT保护柜数量","HUPTProtectCabNum ","个","Num","R","A2"]
[null,null,"高压出线柜数量","HUOutgoingCabNum","个","Num","R","A2"]
[null,null,"高压分段主柜数量","HUSectionMainCabNum","个","Num","R","A2"]
[null,null,"高压分段辅柜数量","HUSectionAssistCabNum","个","Num","R","A2"]
[null,null,"高压备用柜数量","HUBackupCabNum","个","Num","R","A2"]
[null,null,"高压环网柜数量","HURingMainUnitNum","个","Num","R","A2"]
[null,null,"高压双电源开关柜数量","HUDaulPowerSwitchCabNum","个","Num","R","A2"]
[null,"低压","低压变电站类型","LUSubstationType",null,"Enum","M","D1","1. 室内变电站 2. 组合式变电站 3. 预装式变电站 4. 组合式变电器 5. 户外杆上变电台 99. 其他"]
[null,null,"低压主变压器数量","LUMainTransNum","个","Num","S","A2"]
[null,null,"低压主变压器绕组类型","LUMainTransWindingType",null,"Enum","R","D1","1. 双绕组 2. 三绕组 99. 其他"]
[null,null,"低压变电系统额定进线电压 ","LURatedInU","kV","Num","S","A2"]
[null,null,"低压变电系统额定中压出线电压 ","LURatedOutMediumU","kV","Num","S","A2"]
[null,null,"低压变电系统额定低压出线电压 ","LURatedOutLowU","kV","Num","S","A2"]
[null,null,"低压变电系统设计容量","LUDesignCap","kVA","Num","S","A2"]
[null,null,"低压是否为双电源","isLUDualPower",null,"Bool","M","E1","0. 否 1. 是"]
[null,null,"低压双电源运行方式","LUDualPowerOperateType",null,"Enum","M","D1","1. 一用一备 2. 同时运行，互为备用 99. 其他"]
[null,null,"低压开关柜连接关系","LUCabConnect",null,"Topology","R","I"]
[null,null,"低压进线柜数量","LUIncomingCabNum","个","Num","R","A2"]
[null,null,"低压电容补偿柜数量","LUCapCompensationCabNum","个","Num","R","A2"]
[null,null,"低压母联柜数量","LUBusCabNum","个","Num","R","A2"]
[null,null,"低压出线柜（馈电柜）数量","LUOutgoingCabNum","个","Num","R","A2"]
[null,null,"低压计量柜数量","LUMeterCabNum","个","Num","R","A2"]
[null,null,"低压配电接线方式","LUConnectType",null,"Enum","M","D1","1. 单回路树干式 2. 双回路树干式 3. 普通环网式 4. 拉手环网式 5. 链式 6. 单回路放射式 7. 双回路方式 8. 链式 99. 其他"]
[null,null,"低压变压器供电区域","LUSupplyZone",null,"Objects","R","G4"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"本地远程状态","RemoteStatus",null,"Enumv","S","L","1. 本地 2. BA 3. 云端 99. 其他"]
[null,null,"手自动状态","ManualAutoStatus",null,"Boolv","S","L","0. 手动 1. 自动"]
[null,null,"变电系统进线电压 ","InU","kV","Inst","S","L"]
[null,null,"变电系统进线电流","InI","A","Inst","S","L"]
[null,null,"变电系统进线视在功率","InP","kVA","Inst","S","L"]
[null,null,"变电系统进线有功功率","InActiveP","kW","Inst","S","L"]
[null,null,"变电系统进线无功功率","InReactiveP","kVar","Inst","S","L"]
[null,null,"变电系统低压出线电压 ","OutLowU","kV","Inst","S","L"]
[null,null,"变压系统低压出线电流","OutLowI","A","Inst","S","L"]
[null,null,"变电系统低压出线视在功率","OutLowP","kVA","Inst","S","L"]
[null,null,"变电系统低压出线有功功率","InActiveP","kW","Inst","S","L"]
[null,null,"变电系统低压出线无功功率","OutLowReactiveP","kVar","Inst","S","L"]
[null,null,"变电系统中压出线电压 ","OutMediumU","kV","Inst","M","L"]
[null,null,"变电系统中压出线电流","OutMediumI","A","Inst","M","L"]
[null,null,"变电系统中压出线视在功率","OutMediumP","kVA","Inst","M","L"]
[null,null,"变电系统中压出线有功功率","InActiveP","kW","Inst","M","L"]
[null,null,"变电系统中压出线无功功率","OutMediumReactiveP","kVar","Inst","M","L"]
[null,"瞬时指标","低压出线功率因数","OutLowPFactor",null,"Inst","R","L"]
[null,null,"中压出线功率因数","OutMediumPFactor",null,"Inst","R","L"]
[null,null,"变电系统效率","SysEff",null,"Inst","R","M"]
[null,"累计指标","累计视在电能","AccE","kVAh","Acc","M","M"]
[null,null,"累计有功电能","AccActiveE","kWh","Acc","M","M"]
[null,null,"累计无功电能","AccReactiveE","kVarh","Acc","M","M"]
["设定参数"]
["报警消息"]

{"sheet":"DG柴发机房系统","index":1,"n_rows":59,"n_cols":10,"rows_kept":59,"cut":false,"hidden":false,"merged":[[0,0,0,9],[1,0,1,1],[2,1,16,1],[2,0,24,0],[17,1,23,1],[58,0,58,1],[25,0,56,0],[25,1,49,1],[50,1,54,1],[55,1,56,1],[57,0,57,1]]}
["柴发机房系统"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数","柴发机组","使用方式","UseType",null,"Enum","S","D1","1. 常用型 2. 应急型 99. 其他"]
[null,null,"停电瞬间投入时间","SwitchInTime","min","Num","M","A2"]
[null,null,"供电维持时间","LastTime","h","Num","S","A2"]
[null,null,"负担负荷类型","LoadLev",null,"MEnum","S","D2","1. 特别重要负荷 2. 消防负荷及一级负荷 3. 二级负荷 99. 其他 （可多选）"]
[null,null,"柴油发电机台数","DieselGeneratorNum","台","Num","S","A2"]
[null,null,"运行方式","OperateType",null,"Enum","R","D1","1. 单机运行 2. 并机运行 99. 其他"]
[null,null,"额定耗油量","RatedDieselConsum","L/kWh","Num","S","A2"]
[null,null,"常备燃油储量","DieselStoreCap","L","Num","S","A2"]
[null,null,"额定输出电压","RatedOutU","kV","Num","S","A2"]
[null,null,"额定输出电流","RatedOutI","A","Num","M","A2"]
[null,null,"额定输出功率","RatedOutP","kW","Num","S","A2"]
[null,null,"额定发电频率","RatedOutFreq","Hz","Num","M","A2"]
[null,null,"额定功率因数","RatedPFactor",null,"Num","R","A1"]
[null,null,"接地方式","GroundType",null,"MEnum","R","D2","1. 发电机中性点接地（工作接地） 2. 电气设备正常不带电金属外壳接地（保护接地） 3. 防静电接地 99. 其他 （可多选）"]
[null,null,"所在地区海拔","AltitudeType",null,"Bool","R","E1","0. ＜1000米 1. ＞1000米"]
[null,"排风","排烟管道架设方式","ExhaustSmokePipeMode",null,"Enum","R","D1","1. 水平架空 2. 地沟内敷设 99. 其他"]
[null,null,"送风机台数","InFanNum","台","Num","M","A2"]
[null,null,"排风机台数","OutFanNum","台","Num","M","A2"]
[null,null,"排烟机台数","ExhaustSmokeFanNum","台","Num","M","A2"]
[null,null,"额定送风量","RatedAirInFlow","m3/h","Num","M","A2"]
[null,null,"机房换气次数","RatedAirChangeRate","次/h","Num","R","A2"]
[null,null,"额定排烟量","RatedExhaustSmokeFlow","m3/h","Num","M","A2"]
[null,"配电柜","配套低压开关柜数量","LUCabNum","个","Num","M","A2"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"本地远程状态","RemoteStatus",null,"Enumv","S","L","1. 本地 2. BA 3. 云端 99. 其他"]
[null,null,"手自动状态","ManualAutoStatus",null,"Boolv","S","L","0. 手动 1. 自动"]
[null,null,"A相输出电压","APhaseOutU","kV","Inst","M","L"]
[null,null,"B相输出电压","BPhaseOutU","kV","Inst","M","L"]
[null,null,"C相输出电压","CPhaseOutU","kV","Inst","M","L"]
[null,null,"A相输出电流","APhaseOutI","A","Inst","M","L"]
[null,null,"B相输出电流","BPhaseOutI","A","Inst","M","L"]
[null,null,"C相输出电流","CPhaseOutI","A","Inst","M","L"]
[null,null,"A相输出有功功率","APhaseOutActiveP","kW","Inst","M","L"]
[null,null,"B相输出有功功率","BPhaseOutActiveP","kW","Inst","M","L"]
[null,null,"C相输出有功功率","CPhaseOutActiveP","kW","Inst","M","L"]
[null,null,"总输出有功功率","TotOutActiveP","kW","Inst","M","L"]
[null,null,"A相输出无功功率","APhaseOutReactiveP","kVar","Inst","R","L"]
[null,null,"B相输出无功功率","BPhaseOutReactiveP","kVar","Inst","R","L"]
[null,null,"C相输出无功功率","CPhaseOutReactiveP","kVar","Inst","R","L"]
[null,null,"总输出无功功率","TotOutReactiveP","kVar","Inst","R","L"]
[null,null,"A相输出视在功率","APhaseOutApparentP","kVA","Inst","R","L"]
[null,null,"B相输出视在功率","BPhaseOutApparentP","kVA","Inst","R","L"]
[null,null,"C相输出视在功率","CPhaseOutApparentP","kVA","Inst","R","L"]
[null,null,"总输出视在功率","TotOutApparentP","kVA","Inst","R","L"]
[null,null,"输出频率","OutFreq","Hz","Inst","M","L"]
[null,null,"逐时耗燃油量","DieselConsumP","L/h","Inst","S","L"]
[null,null,"油箱储量","DeieselStore","L","Inst","M","L"]
[null,"瞬时指标","A相输出功率因数","APhasePFactor",null,"Inst","R","M"]
[null,null,"B相输出功率因数","BPhasePFactor",null,"Inst","R","M"]
[null,null,"C相输出功率因数","CPhasePFactor",null,"Inst","R","M"]
[null,null,"总输出功率因数","TotPFactor",null,"Inst","R","M"]
[null,null,"单位发电量油耗","UnitEDeieseConsum","L/kWh","Inst","R","M"]
[null,"累计指标","累计发电量","AccOutE","kWh","Acc","M","M"]
[null,null,"累计耗油量","AccDieselConsum","L","Acc","M","M"]
["设定参数"]
["报警消息"]

{"sheet":"BP备用电源系统","index":2,"n_rows":36,"n_cols":10,"rows_kept":36,"cut":false,"hidden":false,"merged":[[34,0,34,1],[35,0,35,1],[0,0,0,9],[1,0,1,1],[2,0,17,0],[2,1,16,1],[18,1,30,1],[18,0,33,0],[32,1,33,1]]}
["备用电源系统"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数","备用电源","备用电源类型 ","BackupPowerType",null,"MEnum ","S","D2","1. UPS 2. EPS 3. 柴油发电机 99. 其他 （可多选）"]
[null,null,"工作原理","PrincipleType",null,"Enum","R","D1","1. 在线式 2. 后备式 3. 在线互动式 99. 其他"]
[null,null,"输出波形","WaveType",null,"Enum","R","D1","1. 正弦波 2. 方波 99. 其他"]
[null,null,"布置形式","LayoutType",null,"Enum","S","D1","1. 集中式 2. 分散式 99. 其他"]
[null,null,"蓄电池类型","BatteryType",null,"Enum","M","D1","1. 铅酸电池 2. 胶体电池 99. 其他"]
[null,null,"额定输入电压","RatedInU","V","Num","M","A2"]
[null,null,"额定输入频率","RatedInFreq","Hz","Num","M","A2"]
[null,null,"额定输出电压","RatedOutU","V","Num","M","A2"]
[null,null,"额定输出频率","RatedOutFreq","Hz","Num","M","A2"]
[null,null,"最大输出功率","MaxOutP","kW","Num","M","A2"]
[null,null,"最大储电容量","MaxElecStore","Ah","Num","M","A2"]
[null,null,"输出维持时间","LastTime","h","Num","S","A2"]
[null,null,"额定电源效率","RatedPowerEff","%","Num","R","A2"]
[null,null,"负担负荷类型","LoadType",null,"MEnum","S","D2","1. 特别重要负荷 2. 消防负荷及一级负荷  2. 二级负荷 99. 其他 （可多选）"]
[null,null,"停电之后的反应机制","ReactionMode",null,"Str","R","B1"]
[null,"配电柜","配套低压开关柜数量","LUCabNum","个","Num","M","A2"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"本地远程状态","RemoteStatus",null,"Enumv","S","L","1. 本地 2. BA 3. 云端 99. 其他"]
[null,null,"手自动状态","ManualAutoStatus",null,"Boolv","S","L","0. 手动 1. 自动"]
[null,null,"供电状态","ElecSupplyStatus",null,"Enumv","S","L","1. 市政正常供电 2. Ups/Eps供电 3. 柴油发电机供电 99. 其他"]
[null,null,"输入电压","InU","V","Inst","M","L"]
[null,null,"输入频率","InFreq","Hz","Inst","M","L"]
[null,null,"输入功率","InP","kW","Inst","M","L"]
[null,null,"输出电压","OutU","V","Inst","M","L"]
[null,null,"输出频率","OutFreq","Hz","Inst","M","L"]
[null,null,"输出功率","OutP","kW","Inst","M","L"]
[null,null,"储电量","EStore","Ah","Inst","M","L"]
[null,null,"频率漂移量","FreqDrift","Hz","Inst","R","L",null,"发电机不稳定造成的电网频率偏差"]
[null,"瞬时指标","电源效率","PowerEff","%","Inst","R","M"]
[null,"累计指标","持续欠压时间","LastUnderUTime","s","Acc","R","M"]
[null,null,"持续过压时间","LastOverUTime","s","Acc","R","M"]
["设定参数"]
["报警消息"]

{"sheet":"EP机房动力系统","index":3,"n_rows":21,"n_cols":10,"rows_kept":21,"cut":false,"hidden":false,"merged":[[20,0,20,1],[0,0,0,9],[1,0,1,1],[2,0,10,1],[11,0,18,1],[19,0,19,1]]}
["机房动力系统"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择","备注"]
["技术参数",null,"负荷级别","LoadLev",null,"Enum","S","D1","1. 一类：需要不间断供电 2. 二类：备用的供电系统 3. 三类：一般用户 99. 其他"]
[null,null,"关联电器工作制度","EquipScheduleType",null,"Enum","S","D1","1. 不间断 2. 工作时间 3. 非工作时间 4. 短时 99. 其他"]
[null,null,"配电支路额定电流","RatedBrI","A","Num","M","A2"]
[null,null,"设计安装功率","DesignP","kW","Num","S","A2"]
[null,null,"继电器过电流值","RelayOverI","A","Num","M","A2",null,"保护电流"]
[null,null,"断路器动作电流","BreakerActionI","A","Num","M","A2"]
[null,null,"关联设备","RelatedEquip",null,"Objects","R","G4"]
[null,null,"开关柜类型","CabType",null,"Enum","R","D1","1. 固定面板式 2. 防护式 3. 抽屉式 99. 其他"]
[null,null,"配套低压开关柜数量","LUCabNum","个","Num","M","A2"]
["运行参数",null,"运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"本地远程状态","RemoteStatus",null,"Enumv","S","L","1. 本地 2. BA 3. 云端 99. 其他"]
[null,null,"手自动状态","ManualAutoStatus",null,"Boolv","S","L","0. 手动 1. 自动"]
[null,null,"支路电压","BrU","V","Inst","S","L"]
[null,null,"支路电流","BrI","A","Inst","M","L"]
[null,null,"支路功率","BrP","kW","Inst","S","L"]
[null,null,"累计用电电能","AccE","kWh","Acc","S","M"]
["设定参数"]
["报警消息"]

{"sheet":"OP室外动力系统","index":4,"n_rows":21,"n_cols":10,"rows_kept":21,"cut":false,"hidden":false,"merged":[[20,0,20,1],[0,0,0,9],[1,0,1,1],[2,0,10,1],[11,0,18,1],[19,0,19,1]]}
["室外动力系统"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择","备注"]
["技术参数",null,"负荷级别","LoadLev",null,"Enum","S","D1","1. 一类：需要不间断供电 2. 二类：备用的供电系统 3. 三类：一般用户 99. 其他"]
[null,null,"关联电器工作制度","EquipScheduleType",null,"Enum","S","D1","1. 不间断 2. 工作时间 3. 非工作时间 4. 短时 99. 其他"]
[null,null,"配电支路额定电流","RatedBrI","A","Num","M","A2"]
[null,null,"设计安装功率","DesignP","kW","Num","S","A2"]
[null,null,"继电器过电流值","RelayOverI","A","Num","M","A2",null,"保护电流"]
[null,null,"断路器动作电流","BreakerActionI","A","Num","M","A2"]
[null,null,"关联设备","RelatedEquip",null,"Objects","R","G4"]
[null,null,"开关柜类型","CabType",null,"Enum","R","D1","1. 固定面板式 2. 防护式 3. 抽屉式 99. 其他"]
[null,null,"配套低压开关柜数量","LUCabNum","个","Num","M","A2"]
["运行参数",null,"运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"本地远程状态","RemoteStatus",null,"Enumv","S","L","1. 本地 2. BA 3. 云端 99. 其他"]
[null,null,"手自动状态","ManualAutoStatus",null,"Boolv","S","L","0. 手动 1. 自动"]
[null,null,"支路电压","BrU","V","Inst","S","L"]
[null,null,"支路电流","BrI","A","Inst","M","L"]
[null,null,"支路功率","BrP","kW","Inst","S","L"]
[null,null,"累计用电电能","AccE","kWh","Acc","S","M"]
["设定参数"]
["报警消息"]

{"sheet":"EL电梯系统","index":5,"n_rows":32,"n_cols":10,"rows_kept":32,"cut":false,"hidden":false,"merged":[[0,0,0,9],[1,0,1,1],[13,1,21,1],[22,0,29,1],[2,1,12,1],[2,0,21,0],[30,0,30,1],[31,0,31,1]]}
["电梯系统"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择","备注"]
["技术参数","电梯","扶梯数量","EscalatorNum","台","Num","S","A2"]
[null,null,"扶梯有无多层跨越","isEscalatorMultilayer",null,"Bool","M","E1","0. 无 1. 有"]
[null,null,"扶梯有无节能状态","isEscalatorESaveMode",null,"Bool","M","E1","0. 无 1. 有"]
[null,null,"客用直梯数量","GuestElevatorNum","台","Num","S","A2"]
[null,null,"货用直梯数量","GoodsElevatorNum","台","Num","S","A2"]
[null,null,"无人时直梯停靠策略","ElevatorVacantStopType",null,"Enum","R","D1","1. 原地停靠 2. 中位层停靠 3. 底层停靠 99. 其他"]
[null,null,"直梯有无联动策略","isElevatorLinkage",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"直梯有无分区","isElevatorPartition",null,"Bool","M","E1","0. 无 1. 有"]
[null,null,"客梯最大承载流量","GuestElevatorMaxFlow","人次/5min","Num","M","A2"]
[null,null,"货梯最大承载流量","GoodsElevatorMaxFlow","kg/5min","Num","M","A2"]
[null,null,"有无消防应急控制措施 ","isEmergencyCtrl",null,"Bool","S","E1","0. 无 1. 有","在消防情况下切断非消防电源"]
[null,"配电柜","负荷级别","LoadLev",null,"Enum","S","D1","1. 一类：需要不间断供电 2. 二类：备用的供电系统 3. 三类：一般用户 99. 其他"]
[null,null,"关联电器工作制度","EquipScheduleType",null,"Enum","S","D1","1. 不间断 2. 工作时间 3. 非工作时间 4. 短时 99. 其他"]
[null,null,"配电支路额定电流","RatedBrI","A","Num","M","A2"]
[null,null,"设计安装功率","DesignP","kW","Num","S","A2"]
[null,null,"继电器过电流值","RelayOverI","A","Num","M","A2",null,"保护电流"]
[null,null,"断路器动作电流","BreakerActionI","A","Num","M","A2"]
[null,null,"关联设备","RelatedEquip",null,"Objects","R","G4"]
[null,null,"开关柜类型","CabType",null,"Enum","R","D1","1. 固定面板式 2. 防护式 3. 抽屉式 99. 其他"]
[null,null,"配套低压开关柜数量","LUCabNum","个","Num","R","A2"]
["运行参数",null,"运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"本地远程状态","RemoteStatus",null,"Enumv","S","L","1. 本地 2. BA 3. 云端 99. 其他"]
[null,null,"手自动状态","ManualAutoStatus",null,"Boolv","S","L","0. 手动 1. 自动"]
[null,null,"支路电压","BrU","V","Inst","M","L"]
[null,null,"支路电流","BrI","A","Inst","M","L"]
[null,null,"支路功率","BrP","kW","Inst","S","L"]
[null,null,"累计用电电能","AccE","kWh","Acc","S","M"]
["设定参数"]
["报警消息"]

{"sheet":"LT照明系统","index":6,"n_rows":30,"n_cols":10,"rows_kept":30,"cut":false,"hidden":false,"merged":[[0,0,0,9],[1,0,1,1],[11,1,19,1],[20,0,27,1],[2,1,10,1],[2,0,19,0],[28,0,28,1],[29,0,29,1]]}
["照明系统"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择","备注"]
["技术参数","灯具","灯具照明类型","LampType",null,"MEnum","R","D2","1. 直接型 2. 半直接型 3. 漫射型 4. 半间接型 5. 间接型 99. 其他 （可多选）"]
[null,null,"功能类型","FuncType",null,"Enum","S","D1","1. 室内公区照明 2. 车库照明 3. 泛光照明 4. 景观照明 5. 广告照明 6. 应急照明 99. 其他"]
[null,null,"节能灯占比","ESaveLampPct","%","Num","R","A2"]
[null,null,"设计照度","DesignLux","lux","Num","S","A2"]
[null,null,"是否分区控制","isZoneCtrl",null,"Bool","S","E1","0. 否 1. 是"]
[null,null,"是否自动控制","isAutoCtrl",null,"Bool","S","E1","0. 否 1. 是"]
[null,null,"自动控制模式","AutoCtrlType",null,"MEnum","M","D2","1. 声控 2. 人员探测控制 3. 定时控制 99. 其他 （可多选）"]
[null,null,"是否有连续调节功能","isContinueAdjust",null,"Bool","S","E1","0. 否 1. 是"]
[null,null,"灯具总功率","RatedTotP","kW","Num","R","A2"]
[null,"配电柜","负荷级别","LoadLev",null,"Enum","S","D1","1. 一类：需要不间断供电 2. 二类：备用的供电系统 3. 三类：一般用户 99. 其他"]
[null,null,"关联电器工作制度","EquipScheduleType",null,"Enum","S","D1","1. 不间断 2. 工作时间 3. 非工作时间 4. 短时 99. 其他"]
[null,null,"配电支路额定电流","RatedBrI","A","Num","M","A2"]
[null,null,"设计安装功率","DesignP","kW","Num","S","A2"]
[null,null,"继电器过电流值","RelayOverI","A","Num","M","A2",null,"保护电流"]
[null,null,"断路器动作电流","BreakerOperateI","A","Num","M","A2"]
[null,null,"关联设备","RelatedEquip",null,"Objects","R","G4"]
[null,null,"开关柜类型","CabType",null,"Enum","R","D1","1. 固定面板式 2. 防护式 3. 抽屉式 99. 其他"]
[null,null,"配套低压开关柜数量","LUCabNum","个","Num","M","A2"]
["运行参数",null,"运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"本地远程状态","RemoteStatus",null,"Enumv","S","L","1. 本地 2. BA 3. 云端 99. 其他"]
[null,null,"手自动状态","ManualAutoStatus",null,"Boolv","S","L","0. 手动 1. 自动"]
[null,null,"支路电压","BrU","V","Inst","M","L"]
[null,null,"支路电流","BrI","A","Inst","M","L"]
[null,null,"支路功率","BrP","kW","Inst","S","L"]
[null,null,"累计用电电能","AccE","kWh","Acc","S","M"]
["设定参数"]
["报警消息"]

{"sheet":"TP租户配电系统","index":7,"n_rows":26,"n_cols":10,"rows_kept":26,"cut":false,"hidden":false,"merged":[[25,0,25,1],[0,0,0,9],[1,0,1,1],[2,0,14,1],[15,0,23,1],[24,0,24,1]]}
["租户配电系统"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择","备注"]
["技术参数",null,"负荷级别","LoadLev",null,"Enum","S","D1","1. 一类：需要不间断供电 2. 二类：备用的供电系统 3. 三类：一般用户 99. 其他"]
[null,null,"关联电器工作制度","EquipScheduleType",null,"Enum","S","D1","1. 不间断 2. 工作时间 3. 非工作时间 4. 短时 99. 其他"]
[null,null,"配电支路额定电流","RatedBrI","A","Num","M","A2"]
[null,null,"设计安装功率","DesignP","kW","Num","S","A2"]
[null,null,"继电器过电流值","RelayOverI","A","Num","S","A2",null,"保护电流"]
[null,null,"断路器动作电流","BreakerActionI","A","Num","S","A2"]
[null,null,"关联设备","RelatedEquip",null,"Objects","R","G4"]
[null,null,"开关柜类型","CabType",null,"Enum","R","D1","1. 固定面板式 2. 防护式 3. 抽屉式 99. 其他"]
[null,null,"配套低压开关柜数量","LUCabNum","个","Num","M","A2"]
[null,null,"租户用电计价方式","TenantChargeType",null,"Enum","S","D1","1. 月账单式 2. 储值卡式 99. 其他"]
[null,null,"是否有峰谷电价","isPVPrice",null,"Bool","S","E1","0. 否 1. 是"]
[null,null,"是否累计分段计价","isAccSectionPrice",null,"Bool","S","E1","0. 否 1. 是"]
[null,null,"电价策略","PriceMode",null,"Str","R","B1"]
["运行参数",null,"运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"本地远程状态","RemoteStatus",null,"Enumv","S","L","1. 本地 2. BA 3. 云端 99. 其他"]
[null,null,"手自动状态","ManualAutoStatus",null,"Boolv","S","L","0. 手动 1. 自动"]
[null,null,"支路电压","BrU","V","Inst","M","L"]
[null,null,"支路电流","BrI","A","Inst","M","L"]
[null,null,"支路功率","BrP","kW","Inst","S","L"]
[null,null,"累计用电电能","AccE","kWh","Acc","S","M"]
[null,null,"累计用电费用","AccCharge","元","Acc","S","M"]
["设定参数"]
["报警消息"]

{"sheet":"SD强电人防系统","index":8,"n_rows":27,"n_cols":10,"rows_kept":27,"cut":false,"hidden":false,"merged":[[26,0,26,1],[0,0,0,9],[1,0,1,1],[2,0,16,1],[17,0,24,1],[25,0,25,1]]}
["强电人防系统"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择","备注"]
["技术参数",null,"战时用途","WartimeFuncType",null,"Enum","S","D1","1. 指挥、通信 2. 中心医院及急救医院 3. 人员掩蔽部 4. 专业队装备部 5. 配套工程 99. 其他"]
[null,null,"人员等级","PersonLev",null,"Enum","S","D1","1. 专业队员 2. 一等人员（局级和局级以上） 3. 二等人员 99. 其他"]
[null,null,"抗力等级","ResistanceLev",null,"Enum","S","D1","1. 1级 2. 2级 3. 2b级 4. 3级 5. 4级 6. 4b级 7. 5级 8. 6级 99. 其他"]
[null,null,"负荷级别","LoadLev",null,"Enum","S","D1","1. 一类：需要不间断供电 2. 二类：备用的供电系统 3. 三类：一般用户 99. 其他"]
[null,null,"防护单元面积","DefenseUnitArea","m2","Num","S","A2",null,"上限800m2"]
[null,null,"关联电器工作制度","EquipScheduleType",null,"Enum","S","D1","1. 不间断 2. 工作时间 3. 非工作时间 4. 短时 99. 其他"]
[null,null,"有无备用电源","isBackupPower",null,"Bool","S","E1","0. 无 1. 有"]
[null,null,"备用电源供电时间","BackupPowerLastTime","h","Num","M","A2"]
[null,null,"配电支路额定电流","RatedBrI","A","Num","R","A2"]
[null,null,"设计安装功率","DesignP","kW","Num","M","A2"]
[null,null,"继电器过电流值","RelayOverI","A","Num","M","A2",null,"保护电流"]
[null,null,"断路器动作电流","BreakerActionI","A","Num","M","A2"]
[null,null,"关联设备","RelatedEquip",null,"Objects","R","G4"]
[null,null,"开关柜类型","CabType",null,"Enum","R","D1","1. 固定面板式 2. 防护式 3. 抽屉式 99. 其他"]
[null,null,"配套低压开关柜数量","LUCabNum","个","Num","R","A2"]
["运行参数",null,"运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"本地远程状态","RemoteStatus",null,"Enumv","S","L","1. 本地 2. BA 3. 云端 99. 其他"]
[null,null,"手自动状态","ManualAutoStatus",null,"Boolv","S","L","0. 手动 1. 自动"]
[null,null,"支路电压","BrU","V","Inst","M","L"]
[null,null,"支路电流","BrI","A","Inst","M","L"]
[null,null,"支路功率","BrP","kW","Inst","S","L"]
[null,null,"累计用电电能","AccE","kWh","Acc","S","M"]
["设定参数"]
["报警消息"]