{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["ADSF人防风机","ADFD滤毒除湿机","ADIO人防风口"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"ADSF人防风机","index":0,"n_rows":76,"n_cols":10,"rows_kept":76,"cut":false,"hidden":false,"merged":[[72,0,74,1],[75,0,75,1],[1,0,1,1],[0,0,0,9],[40,0,71,0],[40,1,61,1],[62,1,66,1],[67,1,71,1],[2,0,39,1]]}
["风机"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"电源频率","PowerFreq ","Hz","Num","M","A2"]
[null,null,"额定电压","RatedU","V","Num","S","A2"]
[null,null,"额定电流","RatedI","A","Num","M","A2"]
[null,null,"额定功率","RatedP","kW","Num","S","A2"]
[null,null,"功能类型","FuncType",null,"Enum","M","D1","1. 送风机 2. 排风机 3. 加压风机 4. 排烟风机 5. 排烟补风机 6. 事故排风机 99. 其他"]
[null,null,"流向类型","DirectionType",null,"Enum","M","D1","1. 离心式 2. 轴流式 3. 贯流式 4. 混流式 99. 其他"]
[null,null,"结构类型","StructureType",null,"Enum","R","D1","1. 单级风机 2. 多级风机 99. 其他"]
[null,null,"压强类型","PressType",null,"Enum","R","D1","1. 通风机 2. 鼓风机 3. 压气机 99. 其他"]
[null,null,"喷嘴类型","NozzleType",null,"Enum","R","D1","1. 万向球形喷嘴 2. 导管式喷嘴 99. 其他","诱导风机"]
[null,null,"喷嘴是否带风量调节阀","isFlowValve",null,"Bool","R","E1","0. 无 1. 有","诱导风机"]
[null,null,"喷口直径","NozzleDiameter","mm","Num","R","A2",null,"诱导风机"]
[null,null,"额定出口风速","RatedAirOutV","m/s","Num","R","A2",null,"诱导风机"]
[null,null,"额定出口风压","RatedAirOutPress","Pa","Num","M","A2",null,"诱导风机"]
[null,null,"额定射程","RatedAirRange","m","Num","M","A2",null,"诱导风机"]
[null,null,"安装类型","InstallType",null,"Enum","R","D1","1. 立式 2. 卧式 3. 立卧两用式 99. 其他"]
[null,null,"额定扬程","RatedHead","Pa","Num","S","A2"]
[null,null,"额定风量","RatedFlow","m3/h","Num","S","A2"]
[null,null,"额定频率","RatedFreq","Hz","Num","R","A2"]
[null,null,"额定转速","RatedRPM","rpm","Num","M","A2"]
[null,null,"风机额定效率","RatedFanEff","%","Num","M","A2"]
[null,null,"电机额定效率","RatedMotorEff","%","Num","R","A2"]
[null,null,"风机调节类型","AdjustType",null,"Enum","S","D1","1. 定频无调节 2. 变频调节 3. 二档调节 4. 三档调节 99. 其他"]
[null,null,"扬程类型","HeadType",null,"Enum","R","D1","1. 高压 2. 中压 3. 低压 99. 其他","离心式：高压范围P>3000Pa，中压范围1000Pa≤P≤3000Pa，低压范围P<1000Pa；轴流式：高压范围P≥500Pa，低压范围P<500Pa"]
[null,null,"旋转方向","RotateType",null,"Enum","R","D1","1. 左式 2. 右式 99. 其他","从主轴槽轮或电动机位置看叶轮旋转方向，逆时针为左式，反之为右式"]
[null,null,"电机传动方式","MotorDriveType",null,"Enum","R","D1","1. 无轴承 2. 悬臂支承，皮带轮在轴承中间 3. 悬臂支承，皮带轮在轴承外侧 4. 悬臂支承，联轴器传动 5. 双支承，皮带在外侧 6. 双支承，联轴器传动 99. 其他"]
[null,null,"风机性能曲线","FanCharacterCurve ",null,"Attachment","R","F1"]
[null,null,"是否有油烟过滤网","isLampblackFilter ",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"工作油烟浓度范围","WorkLampblackRange","mg/m3","Numr","R","A6"]
[null,null,"抗震能力","SeismicCapacity",null,"Enum","S","D1","参考《10抗震设防烈度》"]
[null,null,"电机防护等级","MotorIPGrade",null,"Str","R","B1","参考《11防护等级》"]
[null,null,"电机绝缘等级","MotorInsulationLev",null,"Enum","M","D1","1. Y级 2. A级 3. E级 4. B级 5. F级 6. H级 7. C级 8. N级 9. R级 99. 其他"]
[null,null,"防爆等级","ExplosionProofLev",null,"Enum","M","D1","1. I类 2. II类 2.1 IIA类 2.2 IIB类 2.3 IIC类 3. III类 3.1 IIIA类 3.2 IIIB类 3.3 IIIC类 99. 其他"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"噪声强度","Noise","dB(A)","Num","M","A2"]
[null,null,"振动烈度","Vibration","mm/s","Num","M","A2"]
[null,null,"是否有高海拔要求","isHighAltitude",null,"Bool","R","E1","0. 无高海拔设计 1. 高海拔专用（＞1000米）"]
[null,null,"是否有防盐雾要求","isSaltFogDefend",null,"Bool","R","E1","0. 无防盐雾设计 1. 沿海地区专用"]
[null,null,"能效等级","EEffIndex",null,"Enum","M","D1","1. 1级 2. 2级 3. 3级 4. 4级 5. 5级 99. 其他"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"手自动状态","ManualAutoStatus",null,"Boolv","S","L","0. 手动 1. 自动"]
[null,null,"云端控制状态","InCloudStatus",null,"Boolv","S","L","0. 非云端 1. 云端"]
[null,null,"BA手动干预状态","BAInterveneStatus",null,"Boolv","S","L","0. 不允许 1. 允许"]
[null,null,"A相电压","APhaseU","V","Inst","R","L"]
[null,null,"B相电压","BPhaseU","V","Inst","R","L"]
[null,null,"C相电压","CPhaseU","V","Inst","R","L"]
[null,null,"A相电流","APhaseI","A","Inst","R","L"]
[null,null,"B相电流","BPhaseI","A","Inst","R","L"]
[null,null,"C相电流","CPhaseI","A","Inst","R","L"]
[null,null,"平均电压","U","V","Inst","M"]
[null,null,"平均电流","I","A","Inst","M"]
[null,null,"耗电功率","ElecConsumP","kW","Inst","M","L"]
[null,null,"工作频率","Freq","Hz","Inst","M","L"]
[null,null,"风机转速","FanRPM","rpm","Inst","M","L"]
[null,null,"风机档位","FanGear",null,"Enumv","M","L","1. 低档 2. 中档 3. 高档 99. 其他"]
[null,null,"进风压力","AirInPress","Pa","Inst","R","L"]
[null,null,"出风压力","AirOutPress","Pa","Inst","R","L"]
[null,null,"出口风速","AirOutV",null,"Inst","R","L",null,"诱导风机"]
[null,null,"射程","AirRange",null,"Inst","R","L",null,"诱导风机"]
[null,null,"瞬时风量","AirFlow","m3/h","Inst","M","L"]
[null,"瞬时指标","电流负载率","IPLR","%","Inst","M","M"]
[null,null,"风机效率","FanEff","%","Inst","R","M"]
[null,null,"电机效率","MotorEff","%","Inst","R","M"]
[null,null,"整体效率","OverallEff","%","Inst","R","M"]
[null,null,"风机输配系数","WTFfan",null,"Inst","R","M"]
[null,"累计指标","累计送风量","AccFlow","m3","Acc","R","M"]
[null,null,"累计耗电量","AccElecConsum","kWh","Acc","M","M"]
[null,null,"累计运行时间","AccRunTime","h","Acc","S","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数",null,"设备开关设定","EquipSwitchSet",null,"Boolp","S","L","0. 停止 1. 运行"]
[null,null,"设备频率设定","EquipFreqSet","Hz","Nump","S","L"]
[null,null,"设备档位设定","EquipGearSet",null,"Enump","S","L","1. 低档 2. 中档 3. 高档 99.其他"]
["报警消息"]

{"sheet":"ADFD滤毒除湿机","index":1,"n_rows":41,"n_cols":10,"rows_kept":41,"cut":false,"hidden":false,"merged":[[39,0,39,1],[40,0,40,1],[0,0,0,9],[1,0,1,1],[2,0,13,1],[14,0,38,0],[14,1,31,1],[33,1,38,1]]}
["滤毒除湿机"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"电源频率","PowerFreq ","Hz","Num","M","A2"]
[null,null,"额定电压","RatedU","V","Num","S","A2"]
[null,null,"额定电流","RatedI","A","Num","M","A2"]
[null,null,"额定功率","RatedP","kW","Num","S","A2"]
[null,null,"防护对象","DefenseGasType",null,"MEnum","M","D2","1. 无机气体或蒸汽 2. 有机气体或蒸汽 3. 氨 4. 硫化氢 5. 一氧化碳 6. 酸性气体或蒸汽 99. 其他（可多选）"]
[null,null,"滤毒材质","ChemicalDefenseType",null,"MEnum","M","D2","1. 过滤纸 2. 防毒炭 3. 酶 99. 其他 （可多选）"]
[null,null,"额定净化空气量","RatedAirFlow","m3/h","Num","S","A2"]
[null,null,"额定滤毒效率","RatedChemicalDefenseEff","%","Num","M","A2"]
[null,null,"额定除湿量","RatedDeD","g/h","Num","S","A2"]
[null,null,"适用面积","RatedArea","m2","Num","R","A2"]
[null,null,"抗震能力","SeismicCapacity",null,"Enum","S","D1","参考《10抗震设防烈度》"]
[null,null,"理论压力损失","RatedPressLost","Pa","Num","R","A2"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"手自动状态","ManualAutoStatus",null,"Boolv","S","L","0. 手动 1. 自动"]
[null,null,"云端控制状态","InCloudStatus",null,"Boolv","S","L","0. 非云端 1. 云端"]
[null,null,"BA手动干预状态","BAInterveneStatus",null,"Boolv","S","L","0. 不允许 1. 允许"]
[null,null,"工作电压","U","V","Inst","M","L"]
[null,null,"工作电流","I","A","Inst","M","L"]
[null,null,"耗电功率","ElecConsumP","kW","Inst","M","L"]
[null,null,"净化空气量","AirFlow","m3/h","Inst","M","L"]
[null,null,"进口空气压力","AirInPress","Pa","Inst","R","L"]
[null,null,"出口空气压力","AirOutPress","Pa","Inst","R","L"]
[null,null,"进口空气有毒气体浓度","AirInToxicGas","mol/L","Inst","R","L"]
[null,null,"出口空气有毒气体浓度","AirOutToxicGas ","mol/L","Inst","R","L"]
[null,null,"进口空气温度","AirInTemp","℃","Inst","M","L"]
[null,null,"进口空气相对湿度","AirInRH","%RH","Inst","M","L"]
[null,null,"出口空气温度","AirOutTemp","℃","Inst","M","L"]
[null,null,"出口空气相对湿度","AirOutRH","%RH","Inst","M","L"]
[null,null,"除湿量","DeD","g/h","Inst","M","L"]
[null,"瞬时指标","滤毒效率","ChemicalDefenseEff","%","Inst","R","M"]
[null,"累计指标","累计净化空气量","AccDefenseAir","m3","Acc","R","M"]
[null,null,"累计除湿量","AccDeD","kg","Acc","R","M"]
[null,null,"累计耗电量","AccElecConsum","kWh","Acc","M","M"]
[null,null,"累计运行时间","AccRunTime","h","Acc","S","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]

{"sheet":"ADIO人防风口","index":2,"n_rows":14,"n_cols":10,"rows_kept":14,"cut":false,"hidden":false,"merged":[[0,0,0,9],[12,0,12,1],[13,0,13,1],[1,0,1,1],[8,0,11,1],[2,0,7,1]]}
["风口"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"材质","MaterialType",null,"Enum","R","D1","1. 铁板 2. 镀锌板 3. 铝合金板 4. 不锈钢板 99. 其他"]
[null,null,"类型","StructureType",null,"Enum","M","D1","1. 单层百叶风口 2. 双层百叶风口 3. 固定条形风口 4. 自垂百叶式风口 5. 散流器 6. 球形可调风口 7. 旋流风口 99. 其他"]
[null,null,"形状","ShapeType",null,"Enum","M","D1","1. 正方形 2. 矩形 3. 圆形 99. 其他"]
[null,null,"壁厚","Thick","mm","Num","R","A2"]
[null,null,"抗震能力","SeismicCapacity",null,"Enum","S","D1","参考《10抗震设防烈度》"]
[null,null,"理论压力损失","RatedPressLost","Pa","Num","R","A2"]
["运行参数",null,"进口风压","AirInPress","Pa","Inst","R","L"]
[null,null,"出口风压","AirOutPress","Pa","Inst","R","L"]
[null,null,"瞬时风量","AirFlow","m3/h","Inst","R","L"]
[null,null,"瞬时风温","AirTemp","℃","Inst","R","L"]
["设定参数"]
["报警消息"]