{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["WTWT对讲机","WTRS中继台","WTCU无线对讲控制箱"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"WTWT对讲机","index":0,"n_rows":37,"n_cols":10,"rows_kept":37,"cut":false,"hidden":false,"merged":[[35,0,35,1],[36,0,36,1],[2,0,20,1],[0,0,0,9],[1,0,1,1],[21,0,34,0],[21,1,31,1],[32,1,34,1]]}
["对讲机"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"对讲机类型","RadioType",null,"Enum","S","D1","1. 手持对讲机 2. 车载对讲机 99. 其他"]
[null,null,"供电方式","PowerType",null,"Enum","R","D1","1. 电池式 2. 充电式 3. 直流电源 4. 交流电源 99. 其他"]
[null,null,"额定频率范围","RatedFreqRange","MHz","Num","M","A6"]
[null,null,"频率误差","FreqBias","Hz","Num","R","A2",null,"未调制载波频率与额定（标称）频率之差"]
[null,null,"额定发射功率","RatedTransmitP","W","Num","M","A2",null,"在未加调制情况下，一个射频周期内发射机加给传输线的平均功率"]
[null,null,"发射调制灵敏度","TransmitModulationSensitivity","W","Num","R","A2",null,"使发射机调制频偏达到标准频偏（最大频偏的60%）时的调制信号电平"]
[null,null,"发射调制限制\n(极限调制度)","TransmitModulationLimit","Hz","Num","R","A2",null,"发射机音频电路防止调制频偏超过最大允许偏移的能力"]
[null,null,"音频失真（调制失真）","AudioDistortion","%","Num","R","A2",null,"由于调制电路的非线性而造成的调制音频信号失真"]
[null,null,"调制特性","ModulationCharacter",null,"Str","R","B1",null,"发射机输出信号的频偏跟调制频率的函数关系。衡量发射音频电路是否满足6DB/OCT的预加重特性"]
[null,null,"额定发射信噪比","RatedTransmitSNR","dB(A)","Num","R","A2",null,"在标准调制下，发射机发射出的音频信号和噪声之比，等同于没有任何外部调制信号的情况下,由于哼声和噪声引起的发射机输出信号的调频"]
[null,null,"剩余调频","RestFM","MHz","Num","R","A2",null,"没有任何外部调制信号的情况下由于哼声和噪声引起的发射机输出端信号的调频，衡量指标等同于发射信噪比"]
[null,null,"额定发射机电流","RatedTransmitterI","A","Num","R","A2",null,"发射机处于发射状态时的工作电流值"]
[null,null,"邻道功率","ACP","dB(A)","Num","R","A2",null,"在按信道划分的系统中工作的发射机，在规定的调制条件下总输出功率频谱中落在任何一个相邻信道的规定带宽内的那一部分功率"]
[null,null,"杂散射频分量","SpuriousRadiation","dBm","Num","R","A2",null,"除了载波及其发射带宽附近处的调制分量外，在离散频率上或在窄频带内有一显著分量的信号"]
[null,null,"对讲机使用范围","UseDistance","m","Num","S","A2"]
[null,null,"防护等级","IPGrade",null,"Str","M","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange ","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"在线状态","OnlineStatus",null,"Boolv","S","L","0. 脱线 1. 在线"]
[null,null,"工作状态","WorkStatus",null,"Enumv","M","L","1. 发射 2. 接收 3. 同时收发 4. 待机 99. 其他"]
[null,null,"工作频率","Freq","Hz","Inst","R","L"]
[null,null,"发射功率","TransmitP","W","Inst","R","L"]
[null,null,"接收功率","ReceiveP","W","Inst","R","L"]
[null,null,"发射信噪比","TransmitSNR","dB(A)","Inst","R","L"]
[null,null,"接收信噪比","ReceiveSNR","dB(A)","Inst","R","L"]
[null,null,"发射失真度","TransmitDistortion","%","Inst","R","L"]
[null,null,"接收失真度","ReceiveDistortion","%","Inst","R","L"]
[null,"累计指标","累计运行时间","AccRunTime ","h","Acc","M","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]

{"sheet":"WTRS中继台","index":1,"n_rows":35,"n_cols":10,"rows_kept":35,"cut":false,"hidden":false,"merged":[[33,0,33,1],[34,0,34,1],[0,0,0,9],[1,0,1,1],[19,0,32,0],[19,1,28,1],[14,1,18,1],[29,1,32,1],[2,0,18,0],[2,1,13,1]]}
["中继台"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数","整机","额定电压","RatedU","V","Num","R","A2"]
[null,null,"额定电流","ratedI","A","Num","R","A2"]
[null,null,"额定功率","RatedP","W","Num","R","A2"]
[null,null,"额定发射功率","RatedTransmitP","W","Num","S","A2",null,"在未加调制情况下，一个射频周期内发射机加给传输线的平均功率"]
[null,null,"调制特性","ModulationCharacter",null,"Enum","M","D1","1. PAM 2. PDM 3. PPM 4. PFM 5. PCM 99. 其他"]
[null,null,"接受机灵敏度","ReceiverSensitivity","W","Num","R","A2"]
[null,null,"额定失真度","RatedDistortion","%","Num","R","A2",null,"由于调制电路的非线性而造成的调制音频信号失真"]
[null,null,"调制接受带宽","ModulationBandWidth","Hz","Num","R","A2"]
[null,null,"防护等级","IPGrade",null,"Str","M","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange ","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
[null,"功放","额定输出功率","AmplifierRatedOutP","W","Num","M","A2",null,"指连续的正弦波功率，在1kHz正弦波输入及一定的负载下，\n谐波失真小于1%所输出的功率，表示成W/CH（瓦/声道）"]
[null,null,"总谐波失真","AmplifierTHD","%","Num","R","A2"]
[null,null,"转换率","AmplifierInversion","V/μs","Num","R","A2",null,"单位时间上升的电压幅度"]
[null,null,"阻尼因子","AmplifierDampingFactor",null,"Num","R","A1",null,"功率放大器的负载阻抗（大功率管内部电阻加上音箱的接线线阻）"]
[null,null,"输出阻抗","AmplifieroutImpedance","Ω","Num","R","A2"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"在线状态","OnlineStatus",null,"Boolv","S","L","0. 脱线 1. 在线"]
[null,null,"工作电压","U","V","Inst","R","L"]
[null,null,"工作电流","I","A","Inst","R","L"]
[null,null,"耗电功率","ElecConsumP","W","Inst","R","L"]
[null,null,"工作状态","WorkStatus",null,"Enumv","M","L","1. 发射 2. 接收 3. 同时收发 4. 待机 99. 其他"]
[null,null,"接收功率","ReceiveP","W","Inst","M","L"]
[null,null,"发射功率","TransmitP","W","Inst","M","L",null,"无线电波的发射功率是指在给定频段范围内的能量"]
[null,null,"失真度","Distortion ","%","Inst","R","L"]
[null,"累计指标","累计耗电量","AccElecConsum","kWh","Acc","R","M"]
[null,null,"累计运行时间","AccRunTime","h","Acc","M","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]

{"sheet":"WTCU无线对讲控制箱","index":2,"n_rows":61,"n_cols":10,"rows_kept":61,"cut":false,"hidden":false,"merged":[[60,0,60,1],[1,0,1,1],[18,1,48,1],[49,1,53,1],[2,1,17,1],[0,0,0,9],[2,0,48,0],[49,0,58,0],[54,1,58,1],[59,0,59,1]]}
["控制箱"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数","整机","额定输入电压","RatedInputU","V","Num","R","A2"]
[null,null,"额定输出电压","RatedOutputU","V","Num","R","A2"]
[null,null,"应答时间","ResponseTime","ms","Num","M","A2"]
[null,null,"允许瞬时断电时间","AllowPowerOffTime ","ms","Num","M","A2"]
[null,null,"是否有网络功能","isNetwork",null,"Bool","S","E1","0. 否 1. 是"]
[null,null,"IP地址","IPAddress",null,"Str","S","B1"]
[null,null,"子网掩码","SubnetMask",null,"Str","S","B1"]
[null,null,"网关","Gateway",null,"Str","S","B1"]
[null,null,"DNS服务器地址","DNS",null,"Str","S","B1"]
[null,null,"适用网络类型","NetType",null,"Enum","M","D1","1. 千兆以太网 2. 万兆以太网 3. 光纤 99. 其他"]
[null,null,"传输速率","TransferSpeed","MB/s","Num","M","A2"]
[null,null,"主芯片类型","MainChip",null,"Str","R","B1"]
[null,null,"防护等级","IPGrade",null,"Str","S","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange ","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
[null,"接口","输入485接口数量","In485PortNum","个","Num","R","A2"]
[null,null,"输出485接口数量","Out485PortNum","个","Num","R","A2"]
[null,null,"输入232接口数量","In232PortNum","个","Num","R","A2"]
[null,null,"输出232接口数量","Out232PortNum","个","Num","R","A2"]
[null,null,"输入422接口数量","In422PortNum","个","Num","R","A2"]
[null,null,"输出422接口数量","Out422PortNum","个","Num","R","A2"]
[null,null,"输入MBUS接口数量","InMBUSPortNum","个","Num","R","A2"]
[null,null,"输出MBUS接口数量","OutMBUSPortNum","个","Num","R","A2"]
[null,null,"输入音频接口数量","InAudioPortNum","个","Num","R","A2"]
[null,null,"输出音频接口数量","OutAudioPortNum","个","Num","R","A2"]
[null,null,"HDMI接口数量","HDMIPortNum","个","Num","R","A2"]
[null,null,"VGA接口数量","VGAPortNum","个","Num","R","A2"]
[null,null,"USB接口数量","USBPortNum","个","Num","R","A2"]
[null,null,"以太网接口数量","EthernetPortNum ","个","Num","R","A2"]
[null,null,"光纤接口数量","FiberPortNum ","个","Num","R","A2"]
[null,null,"电压AI接口数量","AIUPortNum","个","Num","R","A2"]
[null,null,"电压AI信号","AIU","V","Num","R","A2"]
[null,null,"电流AI接口数量","AIIPortNum","个","Num","R","A2"]
[null,null,"电流AI信号","AII","A","Num","R","A2"]
[null,null,"电压AO接口数量","AOUPortNum","个","Num","R","A2"]
[null,null,"电压AO信号","AOU","V","Num","R","A2"]
[null,null,"电流AO接口数量","AOIPortNum","个","Num","R","A2"]
[null,null,"电流AO信号","AOI","A","Num","R","A2"]
[null,null,"DI干节点接口数量","DIDryNodePortNum","个","Num","R","A2"]
[null,null,"DI湿节点接口数量","DIWetNodePortNum","个","Num","R","A2"]
[null,null,"DI湿节点电压","DIWetNodeU",null,"Enum","R","D1","1. DC0～30V（标准DC24V） 2. AC110～220V 99. 其他"]
[null,null,"DO干节点接口数量","DODryNodePortNum","个","Num","R","A2"]
[null,null,"DO湿节点接口数量","DOWetNodePortNum","个","Num","R","A2"]
[null,null,"DO湿节点电压","DOWetNodeU",null,"Enum","R","D1","1. DC0～30V（标准DC24V） 2. AC110～220V 99. 其他"]
[null,null,"输入同轴线接口数量","InCoaxialPortNum","个","Num","R","A2"]
[null,null,"输出同轴线接口数量","OutCoaxialPortNum","个","Num","R","A2"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"在线状态","OnlineStatus",null,"Boolv","S","L","0. 脱线 1. 在线"]
[null,null,"上传速度","UploadSpeed","MB/s","Inst","R","L"]
[null,null,"下载速度","DownloadSpeed","MB/s","Inst","R","L"]
[null,"累计指标","累计上传数据量","AccUploadData","GB","Acc","R","L"]
[null,null,"累计下载数据量","AccDownloadData","GB","Acc","R","L"]
[null,null,"累计运行时间","AccRunTime","h","Acc","M","L"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","L"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]