{"text_format":"2","workbook":"xlsx","n_sheets":2,"sheets":["MAHT移动通信信号放大主机","MAAT信号放大天线"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"MAHT移动通信信号放大主机","index":0,"n_rows":42,"n_cols":10,"rows_kept":42,"cut":false,"hidden":false,"merged":[[40,0,40,1],[41,0,41,1],[0,0,0,9],[1,0,1,1],[2,0,27,1],[28,0,39,0],[28,1,35,1],[36,1,39,1]]}
["主机"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"额定电压","RatedU","V","Num","R","A2"]
[null,null,"额定电流","RatedI","A","Num","R","A2"]
[null,null,"额定功率","RatedP","W","Num","R","A2"]
[null,null,"系统类型","OSType",null,"Enum","S","D1","1. Windows 2. Linux 3. IBM-AIX 4. OS X 5. Solaris 6. HP-UX 99. 其他"]
[null,null,"CPU规格","CPUSpecification",null,"Str","M","B1",null,"例：Intel(R)Celeron(R)CPU@1.70GHz "]
[null,null,"CPU个数","CPUNum","个","Num","R","A2"]
[null,null,"CPU频率","CPUFreq","GHz","Num","R","A2"]
[null,null,"内存类型","MemoryType",null,"Enum","R","D1","1. DDR 2. DDR2 3. DDR3 99. 其他"]
[null,null,"内存条数量","MemoryNum","个","Num","R","A2"]
[null,null,"内存大小","MemorySize","MB","Num","M","A2"]
[null,null,"硬盘类型","HardDiskType",null,"MEnum","M","D2","1. SSD 2. SAS 3. NL-SAS 4. SATA 99. 其他 （可多选）"]
[null,null,"硬盘数量","HardDiskNum","个","Num","R","A2"]
[null,null,"硬盘大小","HardDiskSize","GB","Num","M","A2"]
[null,null,"冷却方式","CoolType",null,"Enum","R","D1","1. 水冷 2. 风冷 99. 其他"]
[null,null,"以太网接口数量","EthernetPortNum ","个","Num","R","A2"]
[null,null,"以太网接口速度","EthernetPortSpeed","MB/s","Num","R","A2"]
[null,null,"多媒体接口","MultimediaPort",null,"Str","R","B1"]
[null,null,"IP地址","IPAddress",null,"Str","S","B1"]
[null,null,"子网掩码","SubnetMask",null,"Str","S","B1",null,"用来指明一个IP地址的哪些位标识的是主机所在的子网，以及哪些位标识的是主机的位掩码"]
[null,null,"网关","Gateway",null,"Str","S","B1"]
[null,null,"DNS服务器地址","DNS",null,"Str","S","B1"]
[null,null,"防护等级","IPGrade",null,"Str","S","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange ","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange ","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
[null,null,"能效等级","EEffIndex",null,"Enum","M","D1","1. 1级 2. 2级 3. 3级 4. 4级 5. 5级 99. 其他"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"在线状态","OnlineStatus",null,"Boolv","S","L","0. 脱线 1. 在线"]
[null,null,"工作电压","U","V","Inst","R","L"]
[null,null,"工作电流","I","A","Inst","R","L"]
[null,null,"耗电功率","ElecConsumP","W","Inst","R","L"]
[null,null,"上传速度","UploadSpeed","MB/s","Inst","R","L"]
[null,null,"下载速度","DownloadSpeed","MB/s","Inst","R","L"]
[null,"累计指标","累计耗电量","AccElecConsum","kWh","Acc","R","M"]
[null,null,"累计运行时间","AccRunTime","h","Acc","M","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]

{"sheet":"MAAT信号放大天线","index":1,"n_rows":38,"n_cols":10,"rows_kept":38,"cut":false,"hidden":false,"merged":[[24,1,31,1],[24,0,35,0],[36,0,36,1],[37,0,37,1],[0,0,0,9],[1,0,1,1],[2,0,23,0],[2,1,6,1],[7,1,11,1],[12,1,23,1],[32,1,35,1]]}
["信号放大天线"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数","整机","覆盖范围","CoverArea","m2","Num","S","A2"]
[null,null,"防护等级","IPGrade",null,"Str","S","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange ","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange ","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
[null,"通用电气指标","工作频率范围","FreqRange","Hz","Numr","M","A6"]
[null,null,"输入阻抗","InputR","Ω","Num","R","A2",null,"天线馈电端输入电压与输入电流的比值"]
[null,null,"端口最大输入功率","MaxInputP","W","Num","R","A2"]
[null,null,"电压驻波比","VSWR",null,"Num","R","A1",null,"行波系数的倒数，1~+∞"]
[null,null,"隔离度","IsolationDegree","dB","Num","R","A2",null,"某一极化接收到另一极化信号的比例"]
[null,"空间辐射指标","增益","Gain","dBi","Num","R","A2"]
[null,null,"水平波瓣宽度","HorizontalBeamWidth","°","Num","R","A2"]
[null,null,"垂直波瓣宽度","VerticalBeamWidth","°","Num","R","A2"]
[null,null,"电下倾角","ElecDowntilt","°","Num","R","A2"]
[null,null,"波束下倾角","BeamDip","°","Num","R","A2"]
[null,null,"前后比","FrontBackRatio",null,"Num","R","A1"]
[null,null,"交叉极化比","CrossPolarRatio",null,"Num","R","A1"]
[null,null,"方向图圆度","DirectRoundness","dB","Num","R","A2",null,"全向天线的水平面方向图不圆度是指在水平面方向图中，其最大值或最小值电平值与平均值的偏差。"]
[null,null,"极化方式","PolarType",null,"Enum","R","D1","1. 垂直极化 2. 水平极化 3. +45°斜角 4. -45°斜角 99. 其他"]
[null,null,"交叉极化鉴别率","CrossPolarDetectRatio",null,"Num","R","A1",null,"本信道的主极化分量E11与另一信号在本信道内产生的交叉极化分量E21之比"]
[null,null,"回波损耗","ReturnLoss","dB","Num","R","A2",null,"反射系数绝对值的倒数"]
[null,null,"副瓣抑制","SideBeamRestrain",null,"Str","R","B1",null,"降低旁瓣电平的任何方法、操作或调解"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"在线状态","OnlineStatus",null,"Boolv","S","L","0. 脱线 1. 在线"]
[null,null,"信号输入功率","SignalInputP","W","Inst","M","L"]
[null,null,"信号输出功率","SignalOutputP","W","Inst","M","L"]
[null,null,"工作电压","U","V","Inst","R","L"]
[null,null,"工作电流","I","mA","Inst","R","L"]
[null,null,"耗电功率","ElecConsumP","W","Inst","R","L"]
[null,"累计指标","累计耗电量","AccElecConsum","kWh","Acc","R","M"]
[null,null,"累计运行时间","AccRunTime","h","Acc","M","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]