{"text_format":"2","workbook":"xlsx","n_sheets":8,"sheets":["FAHT火灾报警主机","FADS火灾报警显示屏","FALP联动琴台","FASE火灾探测器","FAAL火灾报警声光报警器","FACU火灾报警控制箱","FAMA消防手动报警按钮","FATL消防电话"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"FAHT火灾报警主机","index":0,"n_rows":42,"n_cols":11,"rows_kept":42,"cut":false,"hidden":false,"merged":[[40,0,40,1],[41,0,41,1],[1,0,1,1],[0,0,0,9],[28,0,39,0],[28,1,35,1],[36,1,39,1],[2,0,27,1]]}
["主机"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"额定电压","RatedU","V","Num","R","A2"]
[null,null,"额定电流","RatedI","A","Num","R","A2"]
[null,null,"额定功率","RatedP","W","Num","R","A2"]
[null,null,"系统类型","OSType",null,"Enum","S","D1","1. Windows 2. Linux 3. IBM-AIX 4. OS X 5. Solaris 6. HP-UX 99. 其他"]
[null,null,"CPU规格","CPUSpecification",null,"Str","M","B1",null,"例：Intel(R)Celeron(R)CPU@1.70GHz "]
[null,null,"CPU个数","CPUNum","个","Num","R","A2"]
[null,null,"CPU频率","CPUFreq","GHz","Num","R","A2"]
[null,null,"内存类型","MemoryType",null,"Enum","R","D1","1. DDR 2. DDR2 3. DDR3 99. 其他"]
[null,null,"内存条数量","MemoryNum","个","Num","R","A2"]
[null,null,"内存大小","MemorySize","MB","Num","M","A2",null,null," "]
[null,null,"硬盘类型","HardDiskType",null,"MEnum","M","D2","1. SSD 2. SAS 3. NL-SAS 4. SATA 99. 其他 （可多选）"]
[null,null,"硬盘数量","HardDiskNum","个","Num","R","A2"]
[null,null,"硬盘大小","HardDiskSize","GB","Num","M","A2"]
[null,null,"冷却方式","CoolType",null,"Enum","R","D1","1. 水冷 2. 风冷 99. 其他"]
[null,null,"以太网接口数量","EthernetPortNum ","个","Num","R","A2"]
[null,null,"以太网接口速度","EthernetPortSpeed","MB/s","Num","R","A2"]
[null,null,"多媒体接口","MultimediaPort",null,"Str","R","B1"]
[null,null,"IP地址","IPAddress",null,"Str","S","B1"]
[null,null,"子网掩码","SubnetMask",null,"Str","S","B1",null,"用来指明一个IP地址的哪些位标识的是主机所在的子网，以及哪些位标识的是主机的位掩码"]
[null,null,"网关","Gateway",null,"Str","S","B1"]
[null,null,"DNS服务器地址","DNS",null,"Str","S","B1"]
[null,null,"防护等级","IPGrade",null,"Str","S","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange ","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange ","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
[null,null,"能效等级","EEffIndex",null,"Enum","M","D1","1. 1级 2. 2级 3. 3级 4. 4级 5. 5级 99. 其他"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"在线状态","OnlineStatus",null,"Boolv","S","L","0. 脱线 1. 在线"]
[null,null,"工作电压","U","V","Inst","R","L"]
[null,null,"工作电流","I","A","Inst","R","L"]
[null,null,"耗电功率","ElecConsumP","W","Inst","R","L"]
[null,null,"上传速度","UploadSpeed","MB/s","Inst","R","L"]
[null,null,"下载速度","DownloadSpeed","MB/s","Inst","R","L"]
[null,"累计指标","累计耗电量","AccElecConsum","kWh","Acc","R","M"]
[null,null,"累计运行时间","AccRunTime","h","Acc","M","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]

{"sheet":"FADS火灾报警显示屏","index":1,"n_rows":45,"n_cols":10,"rows_kept":45,"cut":false,"hidden":false,"merged":[[43,0,43,1],[44,0,44,1],[1,0,1,1],[0,0,0,9],[33,0,42,0],[33,1,38,1],[39,1,42,1],[2,0,32,1]]}
["显示屏"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"额定电压","RatedU","V","Num","R","A2"]
[null,null,"平均功耗","RatedAveP","W","Num","R","A2"]
[null,null,"最大功耗","MaxP","W","Num","R","A2"]
[null,null,"控制系统","CtrlSys",null,"Str","R","B1"]
[null,null,"显示屏类型","DisplayType",null,"Enum","M","D1","1. LED 2. 液晶 99. 其他"]
[null,null,"显示颜色类型","ColorType",null,"Enum","M","D1","1. 单色 2. 双色 3. 彩色 99. 其他"]
[null,null,"显示屏尺寸","DisplaySize","英寸","Num","M","A2"]
[null,null,"有无触摸功能","isTouchFunc",null,"Bool","M","E1","0. 无 1. 有"]
[null,null,"触摸类型","TouchType",null,"Enum","R","D1","1. 单点触摸 2. 多点触摸 99. 其他"]
[null,null,"是否具有红外触摸特性","isIRTouchFunc",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"对比度","Contrast",null,"Num","R","A1"]
[null,null,"亮度","Luminance","cd/m2","Num","R","A2"]
[null,null,"亮度控制","LuminanceCtrl","级","Num","R","A2",null,"8位处理系统256级，矫正4096"]
[null,null,"水平/垂直视角","ViewAngle","°","Num","R","A2"]
[null,null,"支持最大分辨率","MaxResolution",null,"Num","M","A1"]
[null,null,"最佳视距","BestSightDistance","m","Num","R","A2"]
[null,null,"灰度等级","GrayScale",null,"Num","R","A1"]
[null,null,"显示颜色","ColorCap",null,"Num","R","A1"]
[null,null,"字体类型","FontType",null,"Str","R","B1"]
[null,null,"是否有英文显示","isEnglish",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"是否有语音播报功能","isVoiceBroadcastFunc",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"扫描频率","ScanFreq","MHz","Num","R","A2",null,"显示器每秒钟扫描的行数"]
[null,null,"图像传输速度","TransferSpeed","帧/s","Num","R","A2"]
[null,null,"屏幕刷新速率","RefreshRate","Hz","Num","R","A2",null,"显示器的刷新率指每秒钟出现新图像的数量"]
[null,null,"点间距","DotSpace","mm","Num","R","A2",null,"是指一种给定颜色的一个发光点与离它最近的相邻同色发光点之间的距离"]
[null,null,"像素密度","PixelDensity","个/m2","Num","R","A2"]
[null,null,"防护等级","IPGrade",null,"Str","M","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","R","A6"]
[null,null,"工作湿度范围","WorkRHRange ","%RH","Numr","R","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
[null,null,"能效等级","EEffIndex",null,"Enum","M","D1","1. 1级 2. 2级 3. 3级 4. 4级 5. 5级 99. 其他"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"在线状态","OnlineStatus",null,"Boolv","S","L","0. 脱线 1. 在线"]
[null,null,"工作电压","U","V","Inst","R","L"]
[null,null,"工作电流","I","A","Inst","R","L"]
[null,null,"耗电功率","ElecConsumP","W","Inst","R","L"]
[null,"累计指标","累计耗电量","AccElecConsum","kWh","Acc","R","M"]
[null,null,"累计运行时间","AccRunTime","h","Acc","M","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]

{"sheet":"FALP联动琴台","index":2,"n_rows":29,"n_cols":10,"rows_kept":29,"cut":false,"hidden":false,"merged":[[27,0,27,1],[28,0,28,1],[0,0,0,9],[1,0,1,1],[14,0,26,0],[14,1,23,1],[24,1,26,1],[2,0,13,1]]}
["联动琴台"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"额定电压","RatedU","V","Num","R","A2"]
[null,null,"液晶屏规格","ScreenSpecification",null,"Str","M","B1",null,"尺寸"]
[null,null,"地址编码点回路数","AddressIDNodeLoopNum","个","Num","R","A2"]
[null,null,"地址编码点数","AddressIDNodeNum","个","Num","R","A2"]
[null,null,"火灾显示盘数量","FireDisplayPanelNum","个","Num","S","A2"]
[null,null,"联动对象","LinkObject",null,"Objects","R","G4"]
[null,null,"每路输出负载范围","OutLoadRange","Ω","Numr","R","A6"]
[null,null,"通讯方式","CommunicationMode",null,"Str","R","B1"]
[null,null,"防护等级","IPGrade",null,"Str","M","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange","%RH","Numr","R","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"手自动状态","ManualAutoStatus",null,"Boolv","S","L","0. 手动 1. 自动"]
[null,null,"云端控制状态","InCloudStatus",null,"Boolv","S","L","0. 非云端 1. 云端"]
[null,null,"BA手动干预状态","BAInterveneStatus",null,"Boolv","S","L","0. 不允许 1. 允许"]
[null,null,"工作电压","U","V","Inst","R","L"]
[null,null,"工作电流","I","mA","Inst","R","L"]
[null,null,"耗电功率","ElecConsumP","W","Inst","R","L"]
[null,null,"输出负载","OutLoad","Ω","Inst","R","L"]
[null,null,"联动信号","LinkSignal",null,"Boolvs","M","L"]
[null,"累计指标","累计运行时间","AccRunTime","h","Acc","M","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]

{"sheet":"FASE火灾探测器","index":3,"n_rows":41,"n_cols":10,"rows_kept":41,"cut":false,"hidden":false,"merged":[[39,0,39,1],[40,0,40,1],[0,0,0,9],[1,0,1,1],[23,0,38,0],[23,1,35,1],[36,1,38,1],[2,0,22,1]]}
["火灾探测器"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"额定电压","RatedU","V","Num","R","A2"]
[null,null,"监控电流","MonitorI","mA","Num","R","A2"]
[null,null,"报警电流","AlarmI","mA","Num","R","A2"]
[null,null,"探测器类型","DetectorType",null,"MEnum","S","D2","1. 感温探测器 2. 感烟探测器 3. 感可燃气体探测器 4. 感火焰探测器 5. 感光探测器 99. 其他 （可多选）"]
[null,null,"感温探测器定温报警温度限值","TempDetectorAlarmLimit","℃","Num","S","A2"]
[null,null,"感温探测器差温报警温度上升速率限值","TempDetectorAlarmRiseRateLimit","℃/min","Num","S","A2"]
[null,null,"感烟探测器报警浓度","SmokeDetectorAlarmLimit","ppm","Num","S","A4"]
[null,null,"可燃气体探测器气体类型","GasDetectorType ",null,"MEnum","S","D2","1. 液化石油气 2. 天然气 3. 瓦斯 4. 甲苯 5. 煤气 6. 沼气 99. 其他 （可多选）"]
[null,null,"可燃气体探测器报警浓度","GasDetectorAlarmLimit","ppm","Nums","S","A4"]
[null,null,"感光探测器光谱响应范围","LightDetectorSpectrumRange","nm","Numr","S","A6"]
[null,null,"感光探测器报警照度","LightDetectorAlarmLimit","lux","Num","S","A2"]
[null,null,"保护面积","DefenseArea","m2","Num","S","A2"]
[null,null,"报警方式","AlarmType",null,"Enum","M","D1","1. 自带报警器 2. 返回主机报警 99. 其他"]
[null,null,"报警灯光颜色","AlarmLightColor",null,"Str","R","B1",null,"自带报警器"]
[null,null,"报警鸣笛音量","AlarmSoundVolume","dB(A)","Num","R","A2",null,"自带报警器"]
[null,null,"输出信号类型","OutSignalType",null,"Enum","R","D1","1. 开关量 2. 模拟量 3. 数字量 99. 其他"]
[null,null,"信号传输距离","SignalDistance","m","Num","R","A2"]
[null,null,"防护等级","IPGrade",null,"Str","M","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange","%RH","Numr","R","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"手自动状态","ManualAutoStatus",null,"Boolv","S","L","0. 手动 1. 自动"]
[null,null,"云端控制状态","InCloudStatus",null,"Boolv","S","L","0. 非云端 1. 云端"]
[null,null,"BA手动干预状态","BAInterveneStatus",null,"Boolv","S","L","0. 不允许 1. 允许"]
[null,null,"工作电压","U","V","Inst","R","L"]
[null,null,"工作电流","I","mA","Inst","R","L"]
[null,null,"耗电功率","ElecConsumP","W","Inst","R","L"]
[null,null,"探测实时温度","DetectTemp","℃","Inst","R","L"]
[null,null,"探测烟雾浓度","DetectSmoke","ppm","Inst","R","L"]
[null,null,"探测气体浓度","DetectGas","ppm","Insts","R","L"]
[null,null,"探测光谱照度","DetectLux","lux","Inst","R","L"]
[null,null,"报警消息","AlarmMessage",null,"Boolv","S","L"]
[null,"累计指标","累计运行时间","AccRunTime","h","Acc","M","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]

{"sheet":"FAAL火灾报警声光报警器","index":4,"n_rows":25,"n_cols":10,"rows_kept":25,"cut":false,"hidden":false,"merged":[[23,0,23,1],[24,0,24,1],[0,0,0,9],[1,0,1,1],[11,0,22,0],[11,1,19,1],[20,1,22,1],[2,0,10,1]]}
["声光报警器"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"额定电压","RatedU","V","Num","R","A2"]
[null,null,"监控电流","MonitorI","mA","Num","M","A2"]
[null,null,"报警电流","AlarmI","mA","Num","M","A2"]
[null,null,"报警灯光颜色","AlarmLightColor",null,"Str","R","B1"]
[null,null,"报警鸣笛音量","AlarmSoundVolumn","dB(A)","Num","R","A2"]
[null,null,"防护等级","IPGrade",null,"Str","M","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"手自动状态","ManualAutoStatus",null,"Boolv","S","L","0. 手动 1. 自动"]
[null,null,"云端控制状态","InCloudStatus",null,"Boolv","S","L","0. 非云端 1. 云端"]
[null,null,"BA手动干预状态","BAInterveneStatus",null,"Boolv","S","L","0. 不允许 1. 允许"]
[null,null,"工作电压","U","V","Inst","R","L"]
[null,null,"工作电流","I","mA","Inst","R","L"]
[null,null,"耗电功率","ElecConsumP","W","Inst","R","L"]
[null,null,"报警消息","AlarmMessage",null,"Boolv","S","L"]
[null,"累计指标","累计运行时间","AccRunTime","h","Acc","M","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]

{"sheet":"FACU火灾报警控制箱","index":5,"n_rows":61,"n_cols":10,"rows_kept":61,"cut":false,"hidden":false,"merged":[[60,0,60,1],[1,0,1,1],[18,1,48,1],[49,1,53,1],[0,0,0,9],[2,0,48,0],[49,0,58,0],[54,1,58,1],[59,0,59,1],[2,1,17,1]]}
["控制箱"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数","整机","额定输入电压","RatedInputU","V","Num","R","A2"]
[null,null,"额定输出电压","RatedOutputU","V","Num","R","A2"]
[null,null,"应答时间","ResponseTime","ms","Num","M","A2"]
[null,null,"允许瞬时断电时间","AllowPowerOffTime ","ms","Num","M","A2"]
[null,null,"是否有网络功能","isNetwork",null,"Bool","S","E1","0. 否 1. 是"]
[null,null,"IP地址","IPAddress",null,"Str","S","B1"]
[null,null,"子网掩码","SubnetMask",null,"Str","S","B1"]
[null,null,"网关","Gateway",null,"Str","S","B1"]
[null,null,"DNS服务器地址","DNS",null,"Str","S","B1"]
[null,null,"适用网络类型","NetType",null,"Enum","M","D1","1. 千兆以太网 2. 万兆以太网 3. 光纤 99. 其他"]
[null,null,"传输速率","TransferSpeed","MB/s","Num","M","A2"]
[null,null,"主芯片类型","MainChip",null,"Str","R","B1"]
[null,null,"防护等级","IPGrade",null,"Str","S","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange ","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
[null,"接口","输入485接口数量","In485PortNum","个","Num","R","A2"]
[null,null,"输出485接口数量","Out485PortNum","个","Num","R","A2"]
[null,null,"输入232接口数量","In232PortNum","个","Num","R","A2"]
[null,null,"输出232接口数量","Out232PortNum","个","Num","R","A2"]
[null,null,"输入422接口数量","In422PortNum","个","Num","R","A2"]
[null,null,"输出422接口数量","Out422PortNum","个","Num","R","A2"]
[null,null,"输入MBUS接口数量","InMBUSPortNum","个","Num","R","A2"]
[null,null,"输出MBUS接口数量","OutMBUSPortNum","个","Num","R","A2"]
[null,null,"输入音频接口数量","InAudioPortNum","个","Num","R","A2"]
[null,null,"输出音频接口数量","OutAudioPortNum","个","Num","R","A2"]
[null,null,"HDMI接口数量","HDMIPortNum","个","Num","R","A2"]
[null,null,"VGA接口数量","VGAPortNum","个","Num","R","A2"]
[null,null,"USB接口数量","USBPortNum","个","Num","R","A2"]
[null,null,"以太网接口数量","EthernetPortNum ","个","Num","R","A2"]
[null,null,"光纤接口数量","FiberPortNum ","个","Num","R","A2"]
[null,null,"电压AI接口数量","AIUPortNum","个","Num","R","A2"]
[null,null,"电压AI信号","AIU","V","Num","R","A2"]
[null,null,"电流AI接口数量","AIIPortNum","个","Num","R","A2"]
[null,null,"电流AI信号","AII","A","Num","R","A2"]
[null,null,"电压AO接口数量","AOUPortNum","个","Num","R","A2"]
[null,null,"电压AO信号","AOU","V","Num","R","A2"]
[null,null,"电流AO接口数量","AOIPortNum","个","Num","R","A2"]
[null,null,"电流AO信号","AOI","A","Num","R","A2"]
[null,null,"DI干节点接口数量","DIDryNodePortNum","个","Num","R","A2"]
[null,null,"DI湿节点接口数量","DIWetNodePortNum","个","Num","R","A2"]
[null,null,"DI湿节点电压","DIWetNodeU",null,"Enum","R","D1","1. DC0～30V（标准DC24V） 2. AC110～220V 99. 其他"]
[null,null,"DO干节点接口数量","DODryNodePortNum","个","Num","R","A2"]
[null,null,"DO湿节点接口数量","DOWetNodePortNum","个","Num","R","A2"]
[null,null,"DO湿节点电压","DOWetNodeU",null,"Enum","R","D1","1. DC0～30V（标准DC24V） 2. AC110～220V 99. 其他"]
[null,null,"输入同轴线接口数量","InCoaxialPortNum","个","Num","R","A2"]
[null,null,"输出同轴线接口数量","OutCoaxialPortNum","个","Num","R","A2"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"在线状态","OnlineStatus",null,"Boolv","S","L","0. 脱线 1. 在线"]
[null,null,"上传速度","UploadSpeed","MB/s","Inst","R","L"]
[null,null,"下载速度","DownloadSpeed","MB/s","Inst","R","L"]
[null,"累计指标","累计上传数据量","AccUploadData","GB","Acc","R","L"]
[null,null,"累计下载数据量","AccDownloadData","GB","Acc","R","L"]
[null,null,"累计运行时间","AccRunTime","h","Acc","M","L"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","L"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]

{"sheet":"FAMA消防手动报警按钮","index":6,"n_rows":20,"n_cols":10,"rows_kept":20,"cut":false,"hidden":false,"merged":[[18,0,18,1],[19,0,19,1],[17,0,17,1],[2,0,16,1],[0,0,0,9],[1,0,1,1]]}
["手动报警按钮"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"额定电压","RatedU","V","Num","M","A2"]
[null,null,"监视电流","MonitorI","mA","Num","M","A2"]
[null,null,"报警电流","AlarmI","mA","Num","M","A2"]
[null,null,"报警灯光颜色","AlarmLightColor",null,"Str","R","B1"]
[null,null,"报警鸣笛音量","AlarmSoundVolumn","dB(A)","Num","R","A2"]
[null,null,"接线方式","ConnectType",null,"Enum","M","D1","1. 总线制 2. 多线制 99. 其他"]
[null,null,"是否有电话插孔","isTelJack",null,"Bool","M","E1","0. 否 1. 是"]
[null,null,"是否支持编码","isCodingSupport",null,"Bool","R","E1","0. 否 1. 是"]
[null,null,"要求安装高度","RatedInstallHeight","m","Num","M","A2"]
[null,null,"触发方式","TriggerType",null,"Enum","S","D1","1. 玻璃破碎摁钮 2. 可复位报警摁钮 99. 其他"]
[null,null,"复位方式","ResetType",null,"Enum","S","D1","1. 吸盘复位 2. 钥匙复位 3. 更换玻璃复位 99. 其他"]
[null,null,"防护等级","IPGrade",null,"Str","S","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange ","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
["运行参数",null,"报警状态","AlarmStatus",null,"Boolv","S","L","0. 正常 1. 报警"]
["设定参数"]
["报警消息"]

{"sheet":"FATL消防电话","index":7,"n_rows":21,"n_cols":10,"rows_kept":21,"cut":false,"hidden":false,"merged":[[19,0,19,1],[20,0,20,1],[18,0,18,1],[2,0,17,1],[0,0,0,9],[1,0,1,1]]}
["消防电话"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"电话类型","TelType",null,"Enum","S","D1","1. 固定式电话 2. 手提式电话 3. 孔塞式电话 99. 其他"]
[null,null,"供电方式","PowerType",null,"Enum","M","D1","1. 电池式 2. 充电式 3. 直流电源式 4. 交流电源式 99. 其他"]
[null,null,"接线方式","ConnectType",null,"Enum","M","D1","1. 总线制 2. 多线制 99. 其他"]
[null,null,"分机环路最大电阻","MaxR","Ω","Num","R","A2"]
[null,null,"额定频率范围","RatedFreqRange","MHz","Numr","R","A6"]
[null,null,"传输损耗","TransmissionLoss","dB","Num","R","A2"]
[null,null,"杂音电平","NoiseLevel","dB","Num","R","A2"]
[null,null,"发送电平","SendingLevel","dB","Num","R","A2"]
[null,null,"接收电平","ReceivingLevel","dB","Num","R","A2"]
[null,null,"最大串音电平","MaxCrosstalkLevel","dB","Num","R","A2"]
[null,null,"是否具有录音功能","CanRecordSound?",null,"Bool","S","E1","0. 否 1. 是"]
[null,null,"最长录音时间","MaxRrecordingTime","s","Num","M","A2"]
[null,null,"防护等级","IPGrade",null,"Str","S","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange ","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
["运行参数",null,"通话状态","CallStatus",null,"Boolv","S","L","0. 未通话 1. 通话中"]
["设定参数"]
["报警消息"]