{"text_format":"2","workbook":"xlsx","n_sheets":5,"sheets":["BMFE广播前端设备","BMHT广播主机","BMCU广播分区控制箱","BMDS广播显示屏","BMSP扬声器"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"BMFE广播前端设备","index":0,"n_rows":54,"n_cols":10,"rows_kept":54,"cut":false,"hidden":false,"merged":[[52,0,52,1],[53,0,53,1],[49,1,51,1],[0,0,0,9],[35,0,51,0],[1,0,1,1],[32,1,34,1],[25,1,26,1],[11,1,19,1],[27,1,31,1],[20,1,24,1],[2,0,34,0],[35,1,48,1],[2,1,10,1]]}
["广播前端设备"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数","通用","电源频率","PowerFreq","Hz","Num","R","A2"]
[null,null,"额定电压","RatedU","V","Num","R","A2"]
[null,null,"额定电流","RatedI","A","Num","R","A2"]
[null,null,"额定功率","RatedP","W","Num","R","A2"]
[null,null,"功能类型","FuncType",null,"MEnum","S","D2","1. 背景音乐广播 2. 语音广播 3. 紧急广播 99. 其他 （可多选）","火灾或意外事故现场进行应急广播的主要设备，可向现场人员通报事故情况，有效指挥或引导现场人员疏散；非事故情况下也可通过外部输入音源信号（如CD/MP3播放机、调谐器等）进行背景音乐广播"]
[null,null,"防护等级","IPGrade",null,"Str","M","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
[null,"主机","主机信号输入路数","HostInSignalNum","路","Num","R","A2"]
[null,null,"主机线路输入灵敏度","HostInSensitivity","mV","Num","R","A2"]
[null,null,"主机信号输出路数","HostOutSignalNum","路","Num","R","A2"]
[null,null,"主机线路输出电平","HostOutLev","mV","Num","R","A2"]
[null,null,"主机额定输出功率","HostRatedOutP","W","Num","R","A2"]
[null,null,"主机紧急广播触发方式","HostEmergencyTriggerMode",null,"MEnum","S","D2","1. 手动（按下应急键） 2. 自动（输入24V电平） 99. 其他 （可多选）"]
[null,null,"主机失真限制的有效频率范围","HostEffectiveFreqRange  ","kHz","Num","R","A6"]
[null,null,"主机总谐波失真","HostTHD","%","Num","R","A2"]
[null,null,"主机信噪比","HostSNR","dB(A)","Num","R","A2"]
[null,"前置功放","前置功放信号输入路数","PreamplifierInSignalNum","路","Num","R","A2"]
[null,null,"前置功放定压输出","PreamplifierOutU","V","Num","R","A2"]
[null,null,"前置功放额定输出功率","PreamplifierRatedOutP","W","Num","R","A2"]
[null,null,"前置功放信噪比","PreamplifierSNR","dB(A)","Num","R","A2"]
[null,null,"前置功放阻尼因子","PreamplifierDampingFactor",null,"Num","R","A1"]
[null,"矩阵","矩阵信号输入路数","MatrixInSignalNum","路","Num","R","A2"]
[null,null,"矩阵信号输出路数","MatrixOutSignalNum","路","Num","R","A2"]
[null,"功放","功放额定输出功率","AmplifierRatedOutP","W","Num","R","A2",null,"指连续的正弦波功率，在1kHz正弦波输入及一定的负载下，\n谐波失真小于1%所输出的功率，表示成W/CH（瓦/声道）"]
[null,null,"功放总谐波失真","AmplifierTHD","%","Num","R","A2"]
[null,null,"功放转换率","AmplifierConversion","V/μs","Num","R","A2",null,"单位时间上升的电压幅度"]
[null,null,"功放阻尼因子","AmplifierDampingFactor",null,"Num","R","A1"]
[null,null,"功放输出阻抗","AmplifierOutResistance","Ω","Num","R","A2",null,"大功率管内部电阻加上音箱的接线线阻"]
[null,"CD录放盘","CD录放盘最大记录时间段数","CDMaxRecordNum","段","Num","R","A2"]
[null,null,"CD录放盘最大记录时间长度","CDMaxRecordTime","min","Num","R","A2"]
[null,null,"CD录放盘应急广播最大录音时长","CDMaxEmergencyRecordTime","s","Num","M","A2"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"手自动状态","ManualAutoStatus",null,"Boolv","S","L","0. 手动 1. 自动"]
[null,null,"云端控制状态","InCloudStatus",null,"Boolv","S","L","0. 非云端 1. 云端"]
[null,null,"BA手动干预状态","BAInterveneStatus",null,"Boolv","S","L","0. 不允许 1. 允许"]
[null,null,"工作电压","U","V","Inst","R","L"]
[null,null,"工作电流","I","A","Inst","R","L"]
[null,null,"耗电功率","ElecConsumP","W","Inst","R","L"]
[null,null,"输入线连接","InType",null,"Boolv","S","L","0. 其他线路输入 1. 火警触发输入"]
[null,null,"输入电压信号","InSignalU","V","Inst","R","L"]
[null,null,"输出线连接","OutType",null,"Enumv","M","L","1. 线路输出 2. 定压输出 99. 其他","线路输出：此接口用于扩展功率放大器或将音频信号转接至其他音频设备，当本机不能满足现场应用需要时可通过此接口扩展功放，与功放连接线应采用优质屏蔽线；定压输出：定压输出为功率放大器输出，可以直接与定压扬声器连接"]
[null,null,"输出电压信号","OutSignalU","V","Inst","R","L"]
[null,null,"工作频率","Freq","Hz","Inst","R","L"]
[null,null,"负载大小","Load","W","Inst","R","L"]
[null,"累计指标","累计运行时间","AccRunTime","h","Acc","M","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]

{"sheet":"BMHT广播主机","index":1,"n_rows":42,"n_cols":10,"rows_kept":42,"cut":false,"hidden":false,"merged":[[40,0,40,1],[41,0,41,1],[0,0,0,9],[1,0,1,1],[2,0,27,1],[28,0,39,0],[28,1,35,1],[36,1,39,1]]}
["主机"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"额定电压","RatedU","V","Num","R","A2"]
[null,null,"额定电流","RatedI","A","Num","R","A2"]
[null,null,"额定功率","RatedP","W","Num","R","A2"]
[null,null,"系统类型","OSType",null,"Enum","S","D1","1. Windows 2. Linux 3. IBM-AIX 4. OS X 5. Solaris 6. HP-UX 99. 其他"]
[null,null,"CPU规格","CPUSpecification",null,"Str","M","B1",null,"例：Intel(R)Celeron(R)CPU@1.70GHz "]
[null,null,"CPU个数","CPUNum","个","Num","R","A2"]
[null,null,"CPU频率","CPUFreq","GHz","Num","R","A2"]
[null,null,"内存类型","MemoryType",null,"Enum","R","D1","1. DDR 2. DDR2 3. DDR3 99. 其他"]
[null,null,"内存条数量","MemoryNum","个","Num","R","A2"]
[null,null,"内存大小","MemorySize","MB","Num","M","A2"]
[null,null,"硬盘类型","HardDiskType",null,"MEnum","M","D2","1. SSD 2. SAS 3. NL-SAS 4. SATA 99. 其他 （可多选）"]
[null,null,"硬盘数量","HardDiskNum","个","Num","R","A2"]
[null,null,"硬盘大小","HardDiskSize","GB","Num","M","A2"]
[null,null,"冷却方式","CoolType",null,"Enum","R","D1","1. 水冷 2. 风冷 99. 其他"]
[null,null,"以太网接口数量","EthernetPortNum ","个","Num","R","A2"]
[null,null,"以太网接口速度","EthernetPortSpeed","MB/s","Num","R","A2"]
[null,null,"多媒体接口","MultimediaPort",null,"Str","R","B1"]
[null,null,"IP地址","IPAddress",null,"Str","S","B1"]
[null,null,"子网掩码","SubnetMask",null,"Str","S","B1",null,"用来指明一个IP地址的哪些位标识的是主机所在的子网，以及哪些位标识的是主机的位掩码"]
[null,null,"网关","Gateway",null,"Str","S","B1"]
[null,null,"DNS服务器地址","DNS",null,"Str","S","B1"]
[null,null,"防护等级","IPGrade",null,"Str","S","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange ","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange ","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
[null,null,"能效等级","EEffIndex",null,"Enum","M","D1","1. 1级 2. 2级 3. 3级 4. 4级 5. 5级 99. 其他"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"在线状态","OnlineStatus",null,"Boolv","S","L","0. 脱线 1. 在线"]
[null,null,"工作电压","U","V","Inst","R","L"]
[null,null,"工作电流","I","A","Inst","R","L"]
[null,null,"耗电功率","ElecConsumP","W","Inst","R","L"]
[null,null,"上传速度","UploadSpeed","MB/s","Inst","R","L"]
[null,null,"下载速度","DownloadSpeed","MB/s","Inst","R","L"]
[null,"累计指标","累计耗电量","AccElecConsum","kWh","Acc","R","M"]
[null,null,"累计运行时间","AccRunTime","h","Acc","M","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]

{"sheet":"BMCU广播分区控制箱","index":2,"n_rows":61,"n_cols":10,"rows_kept":61,"cut":false,"hidden":false,"merged":[[60,0,60,1],[1,0,1,1],[18,1,48,1],[49,1,53,1],[0,0,0,9],[2,0,48,0],[49,0,58,0],[54,1,58,1],[59,0,59,1],[2,1,17,1]]}
["控制箱"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数","整机","额定输入电压","RatedInputU","V","Num","R","A2"]
[null,null,"额定输出电压","RatedOutputU","V","Num","R","A2"]
[null,null,"应答时间","ResponseTime","ms","Num","M","A2"]
[null,null,"允许瞬时断电时间","AllowPowerOffTime ","ms","Num","M","A2"]
[null,null,"是否有网络功能","isNetwork",null,"Bool","S","E1","0. 否 1. 是"]
[null,null,"IP地址","IPAddress",null,"Str","S","B1"]
[null,null,"子网掩码","SubnetMask",null,"Str","S","B1"]
[null,null,"网关","Gateway",null,"Str","S","B1"]
[null,null,"DNS服务器地址","DNS",null,"Str","S","B1"]
[null,null,"适用网络类型","NetType",null,"Enum","M","D1","1. 千兆以太网 2. 万兆以太网 3. 光纤 99. 其他"]
[null,null,"传输速率","TransferSpeed","MB/s","Num","M","A2"]
[null,null,"主芯片类型","MainChip",null,"Str","R","B1"]
[null,null,"防护等级","IPGrade",null,"Str","S","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange ","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
[null,"接口","输入485接口数量","In485PortNum","个","Num","R","A2"]
[null,null,"输出485接口数量","Out485PortNum","个","Num","R","A2"]
[null,null,"输入232接口数量","In232PortNum","个","Num","R","A2"]
[null,null,"输出232接口数量","Out232PortNum","个","Num","R","A2"]
[null,null,"输入422接口数量","In422PortNum","个","Num","R","A2"]
[null,null,"输出422接口数量","Out422PortNum","个","Num","R","A2"]
[null,null,"输入MBUS接口数量","InMBUSPortNum","个","Num","R","A2"]
[null,null,"输出MBUS接口数量","OutMBUSPortNum","个","Num","R","A2"]
[null,null,"输入音频接口数量","InAudioPortNum","个","Num","R","A2"]
[null,null,"输出音频接口数量","OutAudioPortNum","个","Num","R","A2"]
[null,null,"HDMI接口数量","HDMIPortNum","个","Num","R","A2"]
[null,null,"VGA接口数量","VGAPortNum","个","Num","R","A2"]
[null,null,"USB接口数量","USBPortNum","个","Num","R","A2"]
[null,null,"以太网接口数量","EthernetPortNum ","个","Num","R","A2"]
[null,null,"光纤接口数量","FiberPortNum ","个","Num","R","A2"]
[null,null,"电压AI接口数量","AIUPortNum","个","Num","R","A2"]
[null,null,"电压AI信号","AIU","V","Num","R","A2"]
[null,null,"电流AI接口数量","AIIPortNum","个","Num","R","A2"]
[null,null,"电流AI信号","AII","A","Num","R","A2"]
[null,null,"电压AO接口数量","AOUPortNum","个","Num","R","A2"]
[null,null,"电压AO信号","AOU","V","Num","R","A2"]
[null,null,"电流AO接口数量","AOIPortNum","个","Num","R","A2"]
[null,null,"电流AO信号","AOI","A","Num","R","A2"]
[null,null,"DI干节点接口数量","DIDryNodePortNum","个","Num","R","A2"]
[null,null,"DI湿节点接口数量","DIWetNodePortNum","个","Num","R","A2"]
[null,null,"DI湿节点电压","DIWetNodeU",null,"Enum","R","D1","1. DC0～30V（标准DC24V） 2. AC110～220V 99. 其他"]
[null,null,"DO干节点接口数量","DODryNodePortNum","个","Num","R","A2"]
[null,null,"DO湿节点接口数量","DOWetNodePortNum","个","Num","R","A2"]
[null,null,"DO湿节点电压","DOWetNodeU",null,"Enum","R","D1","1. DC0～30V（标准DC24V） 2. AC110～220V 99. 其他"]
[null,null,"输入同轴线接口数量","InCoaxialPortNum","个","Num","R","A2"]
[null,null,"输出同轴线接口数量","OutCoaxialPortNum","个","Num","R","A2"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"在线状态","OnlineStatus",null,"Boolv","S","L","0. 脱线 1. 在线"]
[null,null,"上传速度","UploadSpeed","MB/s","Inst","R","L"]
[null,null,"下载速度","DownloadSpeed","MB/s","Inst","R","L"]
[null,"累计指标","累计上传数据量","AccUploadData","GB","Acc","R","L"]
[null,null,"累计下载数据量","AccDownloadData","GB","Acc","R","L"]
[null,null,"累计运行时间","AccRunTime","h","Acc","M","L"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","L"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]

{"sheet":"BMDS广播显示屏","index":3,"n_rows":45,"n_cols":10,"rows_kept":45,"cut":false,"hidden":false,"merged":[[43,0,43,1],[44,0,44,1],[0,0,0,9],[1,0,1,1],[2,0,32,1],[33,0,42,0],[33,1,38,1],[39,1,42,1]]}
["显示屏"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"额定电压","RatedU","V","Num","R","A2"]
[null,null,"平均功耗","RatedAveP","W","Num","R","A2"]
[null,null,"最大功耗","MaxP","W","Num","R","A2"]
[null,null,"控制系统","CtrlSys",null,"Str","R","B1"]
[null,null,"显示屏类型","DisplayType",null,"Enum","M","D1","1. LED 2. 液晶 99. 其他"]
[null,null,"显示颜色类型","ColorType",null,"Enum","M","D1","1. 单色 2. 双色 3. 彩色 99. 其他"]
[null,null,"显示屏尺寸","DisplaySize","英寸","Num","M","A2"]
[null,null,"有无触摸功能","isTouchFunc",null,"Bool","M","E1","0. 无 1. 有"]
[null,null,"触摸类型","TouchType",null,"Enum","R","D1","1. 单点触摸 2. 多点触摸 99. 其他"]
[null,null,"是否具有红外触摸特性","isIRTouchFunc",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"对比度","Contrast",null,"Num","R","A1"]
[null,null,"亮度","Luminance","cd/m2","Num","R","A2"]
[null,null,"亮度控制","LuminanceCtrl","级","Num","R","A2",null,"8位处理系统256级，矫正4096"]
[null,null,"水平/垂直视角","ViewAngle","°","Num","R","A2"]
[null,null,"支持最大分辨率","MaxResolution",null,"Num","M","A1"]
[null,null,"最佳视距","BestSightDistance","m","Num","R","A2"]
[null,null,"灰度等级","GrayScale",null,"Num","R","A1"]
[null,null,"显示颜色","ColorCap",null,"Num","R","A1"]
[null,null,"字体类型","FontType",null,"Str","R","B1"]
[null,null,"是否有英文显示","isEnglish",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"是否有语音播报功能","isVoiceBroadcastFunc",null,"Bool","R","E1","0. 无 1. 有"]
[null,null,"扫描频率","ScanFreq","MHz","Num","R","A2",null,"显示器每秒钟扫描的行数"]
[null,null,"图像传输速度","TransferSpeed","帧/s","Num","R","A2"]
[null,null,"屏幕刷新速率","RefreshRate","Hz","Num","R","A2",null,"显示器的刷新率指每秒钟出现新图像的数量"]
[null,null,"点间距","DotSpace","mm","Num","R","A2",null,"是指一种给定颜色的一个发光点与离它最近的相邻同色发光点之间的距离"]
[null,null,"像素密度","PixelDensity","个/m2","Num","R","A2"]
[null,null,"防护等级","IPGrade",null,"Str","M","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange ","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
[null,null,"能效等级","EEffIndex",null,"Enum","M","D1","1. 1级 2. 2级 3. 3级 4. 4级 5. 5级 99. 其他"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"在线状态","OnlineStatus",null,"Boolv","S","L","0. 脱线 1. 在线"]
[null,null,"工作电压","U","V","Inst","R","L"]
[null,null,"工作电流","I","A","Inst","R","L"]
[null,null,"耗电功率","ElecConsumP","W","Inst","R","L"]
[null,"累计指标","累计耗电量","AccElecConsum","kWh","Acc","R","M"]
[null,null,"累计运行时间","AccRunTime","h","Acc","M","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]

{"sheet":"BMSP扬声器","index":4,"n_rows":32,"n_cols":10,"rows_kept":32,"cut":false,"hidden":false,"merged":[[30,0,30,1],[31,0,31,1],[0,0,0,9],[1,0,1,1],[17,0,29,0],[17,1,25,1],[26,1,29,1],[2,0,16,1]]}
["扬声器"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"电源频率","PowerFreq","Hz","Num","M","A2"]
[null,null,"额定电压","RatedU","V","Num","S","A2"]
[null,null,"额定电流","RatedI","A","Num","M","A2"]
[null,null,"额定功率","RatedP","W","Num","S","A2"]
[null,null,"类型","SpeakerType",null,"Enum","M","D1","1. 天花吸顶式 2. 室外音柱式 3. 草坪音箱式 99. 其他"]
[null,null,"额定阻抗","RatedResistance","Ω","Num","R","A2"]
[null,null,"额定信噪比","RatedSNR","dB(A)","Num","R","A2"]
[null,null,"频率响应范围","FreqResponseRange","Hz","Numr","R","A6"]
[null,null,"额定共振频率","RatedResonanceFreq","Hz","Num","R","A2",null,"在扬声器单元的阻抗模值随频率递增变\n化的曲线上，出现一个阻抗极大值时所对应的频率"]
[null,null,"谐波失真","THD","%","Num","R","A2"]
[null,null,"防护等级","IPGrade",null,"Str","M","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
[null,null,"能效等级","EEffIndex",null,"Enum","M","D1","1. 1级 2. 2级 3. 3级 4. 4级 5. 5级 99. 其他"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"手自动状态","ManualAutoStatus",null,"Boolv","S","L","0. 手动 1. 自动"]
[null,null,"云端控制状态","InCloudStatus",null,"Boolv","S","L","0. 非云端 1. 云端"]
[null,null,"BA手动干预状态","BAInterveneStatus",null,"Boolv","S","L","0. 不允许 1. 允许"]
[null,null,"工作电压","U","V","Inst","R","L"]
[null,null,"工作电流","I","A","Inst","R","L"]
[null,null,"耗电功率","ElecConsumP","W","Inst","R","L"]
[null,null,"信噪比","SNR","dB(A)","Inst","R","L"]
[null,"累计指标","累计耗电量","AccElecConsum","kWh","Acc","R","M"]
[null,null,"累计运行时间","AccRunTime","h","Acc","M","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]