{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["KECU厨房自动灭火控制箱","KEEC厨房自动灭火灭火剂容器","KESN厨房自动灭火喷头"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"KECU厨房自动灭火控制箱","index":0,"n_rows":61,"n_cols":10,"rows_kept":61,"cut":false,"hidden":false,"merged":[[59,0,59,1],[60,0,60,1],[0,0,0,9],[1,0,1,1],[2,0,48,0],[2,1,17,1],[18,1,48,1],[49,0,58,0],[49,1,53,1],[54,1,58,1]]}
["控制箱"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数","整机","额定输入电压","RatedInputU","V","Num","R","A2"]
[null,null,"额定输出电压","RatedOutputU","V","Num","R","A2"]
[null,null,"应答时间","ResponseTime","ms","Num","M","A2"]
[null,null,"允许瞬时断电时间","AllowPowerOffTime ","ms","Num","M","A2"]
[null,null,"是否有网络功能","isNetwork",null,"Bool","S","E1","0. 否 1. 是"]
[null,null,"IP地址","IPAddress",null,"Str","S","B1"]
[null,null,"子网掩码","SubnetMask",null,"Str","S","B1"]
[null,null,"网关","Gateway",null,"Str","S","B1"]
[null,null,"DNS服务器地址","DNS",null,"Str","S","B1"]
[null,null,"适用网络类型","NetType",null,"Enum","M","D1","1. 千兆以太网 2. 万兆以太网 3. 光纤 99. 其他"]
[null,null,"传输速率","TransferSpeed","MB/s","Num","M","A2"]
[null,null,"主芯片类型","MainChip",null,"Str","R","B1"]
[null,null,"防护等级","IPGrade",null,"Str","S","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange ","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
[null,"接口","输入485接口数量","In485PortNum","个","Num","R","A2"]
[null,null,"输出485接口数量","Out485PortNum","个","Num","R","A2"]
[null,null,"输入232接口数量","In232PortNum","个","Num","R","A2"]
[null,null,"输出232接口数量","Out232PortNum","个","Num","R","A2"]
[null,null,"输入422接口数量","In422PortNum","个","Num","R","A2"]
[null,null,"输出422接口数量","Out422PortNum","个","Num","R","A2"]
[null,null,"输入MBUS接口数量","InMBUSPortNum","个","Num","R","A2"]
[null,null,"输出MBUS接口数量","OutMBUSPortNum","个","Num","R","A2"]
[null,null,"输入音频接口数量","InAudioPortNum","个","Num","R","A2"]
[null,null,"输出音频接口数量","OutAudioPortNum","个","Num","R","A2"]
[null,null,"HDMI接口数量","HDMIPortNum","个","Num","R","A2"]
[null,null,"VGA接口数量","VGAPortNum","个","Num","R","A2"]
[null,null,"USB接口数量","USBPortNum","个","Num","R","A2"]
[null,null,"以太网接口数量","EthernetPortNum ","个","Num","R","A2"]
[null,null,"光纤接口数量","FiberPortNum ","个","Num","R","A2"]
[null,null,"电压AI接口数量","AIUPortNum","个","Num","R","A2"]
[null,null,"电压AI信号","AIU","V","Num","R","A2"]
[null,null,"电流AI接口数量","AIIPortNum","个","Num","R","A2"]
[null,null,"电流AI信号","AII","A","Num","R","A2"]
[null,null,"电压AO接口数量","AOUPortNum","个","Num","R","A2"]
[null,null,"电压AO信号","AOU","V","Num","R","A2"]
[null,null,"电流AO接口数量","AOIPortNum","个","Num","R","A2"]
[null,null,"电流AO信号","AOI","A","Num","R","A2"]
[null,null,"DI干节点接口数量","DIDryNodePortNum","个","Num","R","A2"]
[null,null,"DI湿节点接口数量","DIWetNodePortNum","个","Num","R","A2"]
[null,null,"DI湿节点电压","DIWetNodeU",null,"Enum","R","D1","1. DC0～30V（标准DC24V） 2. AC110～220V 99. 其他"]
[null,null,"DO干节点接口数量","DODryNodePortNum","个","Num","R","A2"]
[null,null,"DO湿节点接口数量","DOWetNodePortNum","个","Num","R","A2"]
[null,null,"DO湿节点电压","DOWetNodeU",null,"Enum","R","D1","1. DC0～30V（标准DC24V） 2. AC110～220V 99. 其他"]
[null,null,"输入同轴线接口数量","InCoaxialPortNum","个","Num","R","A2"]
[null,null,"输出同轴线接口数量","OutCoaxialPortNum","个","Num","R","A2"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"在线状态","OnlineStatus",null,"Boolv","S","L","0. 脱线 1. 在线"]
[null,null,"上传速度","UploadSpeed","MB/s","Inst","R","L"]
[null,null,"下载速度","DownloadSpeed","MB/s","Inst","R","L"]
[null,"累计指标","累计上传数据量","AccUploadData","GB","Acc","R","L"]
[null,null,"累计下载数据量","AccDownloadData","GB","Acc","R","L"]
[null,null,"累计运行时间","AccRunTime","h","Acc","M","L"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","L"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]

{"sheet":"KEEC厨房自动灭火灭火剂容器","index":1,"n_rows":29,"n_cols":10,"rows_kept":29,"cut":false,"hidden":false,"merged":[[27,0,27,1],[28,0,28,1],[0,0,0,9],[1,0,1,1],[2,0,13,1],[14,0,26,0],[14,1,23,1],[24,1,26,1]]}
["灭火剂容器"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"灭火剂类型","ExtinguishantType",null,"Bool","S","E1","0. 食用油专用灭火剂 1. 其他灭火剂"]
[null,null,"瓶组类型","BottleGroupType",null,"Enum","M","D1","1. 单瓶组 2. 双瓶组 99. 其他"]
[null,null,"灭火剂贮存类型","ExtinguishantStorageType",null,"Enum","M","D1","1. 贮压式 2. 贮气瓶驱动式 99. 其他"]
[null,null,"灭火剂贮存压力","ExtinguishantStoragePress","MPa","Num","R","A2"]
[null,null,"灭火剂有效期限","ExtinguishantValidTime","年","Num","M","A2"]
[null,null,"单个灭火瓶容积","SingleCylinderCap","L","Num","R","A2"]
[null,null,"灭火剂充装密度","ExtinguishantFillDensity","kg/m3","Num","R","A2"]
[null,null,"灭火剂喷射时间","ExtinguishantSprayTime","s","Num","M","A2"]
[null,null,"驱动气体","DriveGasType",null,"Enum","R","D1","1. 氮气 99. 其他","贮气瓶驱动式灭火瓶系列"]
[null,null,"启动方式","StartType",null,"Enum","R","D1","1. 电启动 2. 机械启动 99. 其他"]
[null,null,"驱动气体贮存压力","DriveGasStoragePress","MPa","Num","R","A2"]
[null,null,"驱动气体泄放动作压力","DriveGasStartPress","MPa","Num","R","A2"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"手自动状态","ManualAutoStatus",null,"Boolv","S","L","0. 手动 1. 自动"]
[null,null,"云端控制状态","InCloudStatus",null,"Boolv","S","L","0. 非云端 1. 云端"]
[null,null,"BA手动干预状态","BAInterveneStatus",null,"Boolv","S","L","0. 不允许 1. 允许"]
[null,null,"出口流量","OutFlow","L/s","Inst","M","L"]
[null,null,"出口压力","OutPress","MPa","Inst","M","L"]
[null,null,"瓶内压力","InPress","MPa","Inst","S","L"]
[null,null,"瓶内气体储量","InGasStore","%","Inst","S","L"]
[null,null,"瓶内温度","InGasTemp","℃","Inst","M","L"]
[null,"累计指标","累计运行时间","AccRunTime","h","Acc","R","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]

{"sheet":"KESN厨房自动灭火喷头","index":2,"n_rows":30,"n_cols":10,"rows_kept":30,"cut":false,"hidden":false,"merged":[[28,0,28,1],[29,0,29,1],[0,0,0,9],[1,0,1,1],[2,0,12,1],[13,0,27,0],[13,1,23,1],[24,1,27,1]]}
["喷头"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"功能类型","FuncType",null,"Enum","S","D1","1. 喷灌喷头 2. 水景喷头 99. 其他"]
[null,null,"喷头类型","NozzleType",null,"Enum","M","D1","1. 庭院喷头 2. 地埋式喷头 3. 摇臂式喷头 99. 其他","喷灌喷头"]
[null,null,"喷洒方式","SprayType",null,"Enum","R","D1","1. 散射 2. 射线 3. 旋转 4. 射线旋转 99. 其他","喷灌喷头"]
[null,null,"喷射形状","ShapeType",null,"Enum","R","D1","1. 万向直流 2. 旋转 3. 凤尾 4. 集束 5. 礼花 6. 半球 7. 环形 8. 扇形 9. 蒲公英 10. 半蒲公英 11. 玉柱 12. 雪松 13. 涌泉 14. 水雾 99. 其它","水景喷头"]
[null,null,"喷嘴直径","NozzleDiameter","mm","Num","M","A2"]
[null,null,"额定出水量","RatedWaterOutFlow","m3/h","Num","M","A2"]
[null,null,"额定出水流速","RatedWaterOutV","m/s","Num","M","A2"]
[null,null,"额定射程","RatedSprayRange","m","Num","R","A2"]
[null,null,"理论压损","RatedPressLoss","MPa","Num","R","A2"]
[null,null,"喷洒扇形角度","MaxSprayAngle","°","Num","R","A2"]
[null,null,"喷嘴材质","NozzleMaterial",null,"Enum","R","D1","1. 黄铜 2. 不锈钢 99. 其他"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"手自动状态","ManualAutoStatus",null,"Boolv","S","L","0. 手动 1. 自动"]
[null,null,"云端控制状态","InCloudStatus",null,"Boolv","S","L","0. 非云端 1. 云端"]
[null,null,"BA手动干预状态","BAInterveneStatus",null,"Boolv","S","L","0. 不允许 1. 允许"]
[null,null,"出水流量","WaterOutFlow","m3/h","Inst","R","L"]
[null,null,"出口流速","WaterOutV","m/s","Inst","R","L"]
[null,null,"出水压力","WaterOutPress","MPa","Inst","R","L"]
[null,null,"出水温度","WaterOutTemp","℃","Inst","R","L"]
[null,null,"射程","SprayRange","m","Inst","R","M"]
[null,null,"阀门开度","ValveOpening","%","Inst","M","L"]
[null,"累计指标","累计出水量","AccSprayVolume","m3","Acc","R","M"]
[null,null,"累计运行时间","AccRunTime","h","Acc","R","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]