{"text_format":"2","workbook":"xlsx","n_sheets":4,"sheets":["EGHT门禁主机","EGCU门禁控制箱","EGCR门禁读卡器","EGFG速通门"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"EGHT门禁主机","index":0,"n_rows":42,"n_cols":10,"rows_kept":42,"cut":false,"hidden":false,"merged":[[40,0,40,1],[41,0,41,1],[1,0,1,1],[0,0,0,9],[28,0,39,0],[28,1,35,1],[36,1,39,1],[2,0,27,1]]}
["主机"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"额定电压","RatedU","V","Num","R","A2"]
[null,null,"额定电流","RatedI","A","Num","R","A2"]
[null,null,"额定功率","RatedP","W","Num","R","A2"]
[null,null,"系统类型","OSType",null,"Enum","S","D1","1. Windows 2. Linux 3. IBM-AIX 4. OS X 5. Solaris 6. HP-UX 99. 其他"]
[null,null,"CPU规格","CPUSpecification",null,"Str","M","B1",null,"例：Intel(R)Celeron(R)CPU@1.70GHz "]
[null,null,"CPU个数","CPUNum","个","Num","R","A2"]
[null,null,"CPU频率","CPUFreq","GHz","Num","R","A2"]
[null,null,"内存类型","MemoryType",null,"Enum","R","D1","1. DDR 2. DDR2 3. DDR3 99. 其他"]
[null,null,"内存条数量","MemoryNum","个","Num","R","A2"]
[null,null,"内存大小","MemorySize","MB","Num","M","A2"]
[null,null,"硬盘类型","HardDiskType",null,"MEnum","M","D2","1. SSD 2. SAS 3. NL-SAS 4. SATA 99. 其他 （可多选）"]
[null,null,"硬盘数量","HardDiskNum","个","Num","R","A2"]
[null,null,"硬盘大小","HardDiskSize","GB","Num","M","A2"]
[null,null,"冷却方式","CoolType",null,"Enum","R","D1","1. 水冷 2. 风冷 99. 其他"]
[null,null,"以太网接口数量","EthernetPortNum ","个","Num","R","A2"]
[null,null,"以太网接口速度","EthernetPortSpeed","MB/s","Num","R","A2"]
[null,null,"多媒体接口","MultimediaPort",null,"Str","R","B1"]
[null,null,"IP地址","IPAddress",null,"Str","S","B1"]
[null,null,"子网掩码","SubnetMask",null,"Str","S","B1",null,"用来指明一个IP地址的哪些位标识的是主机所在的子网，以及哪些位标识的是主机的位掩码"]
[null,null,"网关","Gateway",null,"Str","S","B1"]
[null,null,"DNS服务器地址","DNS",null,"Str","S","B1"]
[null,null,"防护等级","IPGrade",null,"Str","S","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange ","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange ","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
[null,null,"能效等级","EEffIndex",null,"Enum","M","D1","1. 1级 2. 2级 3. 3级 4. 4级 5. 5级 99. 其他"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"在线状态","OnlineStatus",null,"Boolv","S","L","0. 脱线 1. 在线"]
[null,null,"工作电压","U","V","Inst","R","L"]
[null,null,"工作电流","I","A","Inst","R","L"]
[null,null,"耗电功率","ElecConsumP","W","Inst","R","L"]
[null,null,"上传速度","UploadSpeed","MB/s","Inst","R","L"]
[null,null,"下载速度","DownloadSpeed","MB/s","Inst","R","L"]
[null,"累计指标","累计耗电量","AccElecConsum","kWh","Acc","R","M"]
[null,null,"累计运行时间","AccRunTime","h","Acc","M","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]

{"sheet":"EGCU门禁控制箱","index":1,"n_rows":61,"n_cols":10,"rows_kept":61,"cut":false,"hidden":false,"merged":[[60,0,60,1],[1,0,1,1],[18,1,48,1],[49,1,53,1],[0,0,0,9],[2,0,48,0],[49,0,58,0],[54,1,58,1],[59,0,59,1],[2,1,17,1]]}
["控制箱"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数","整机","额定输入电压","RatedInputU","V","Num","R","A2"]
[null,null,"额定输出电压","RatedOutputU","V","Num","R","A2"]
[null,null,"应答时间","ResponseTime","ms","Num","M","A2"]
[null,null,"允许瞬时断电时间","AllowPowerOffTime ","ms","Num","M","A2"]
[null,null,"是否有网络功能","isNetwork",null,"Bool","S","E1","0. 否 1. 是"]
[null,null,"IP地址","IPAddress",null,"Str","S","B1"]
[null,null,"子网掩码","SubnetMask",null,"Str","S","B1"]
[null,null,"网关","Gateway",null,"Str","S","B1"]
[null,null,"DNS服务器地址","DNS",null,"Str","S","B1"]
[null,null,"适用网络类型","NetType",null,"Enum","M","D1","1. 千兆以太网 2. 万兆以太网 3. 光纤 99. 其他"]
[null,null,"传输速率","TransferSpeed","MB/s","Num","M","A2"]
[null,null,"主芯片类型","MainChip",null,"Str","R","B1"]
[null,null,"防护等级","IPGrade",null,"Str","S","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange ","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
[null,"接口","输入485接口数量","In485PortNum","个","Num","R","A2"]
[null,null,"输出485接口数量","Out485PortNum","个","Num","R","A2"]
[null,null,"输入232接口数量","In232PortNum","个","Num","R","A2"]
[null,null,"输出232接口数量","Out232PortNum","个","Num","R","A2"]
[null,null,"输入422接口数量","In422PortNum","个","Num","R","A2"]
[null,null,"输出422接口数量","Out422PortNum","个","Num","R","A2"]
[null,null,"输入MBUS接口数量","InMBUSPortNum","个","Num","R","A2"]
[null,null,"输出MBUS接口数量","OutMBUSPortNum","个","Num","R","A2"]
[null,null,"输入音频接口数量","InAudioPortNum","个","Num","R","A2"]
[null,null,"输出音频接口数量","OutAudioPortNum","个","Num","R","A2"]
[null,null,"HDMI接口数量","HDMIPortNum","个","Num","R","A2"]
[null,null,"VGA接口数量","VGAPortNum","个","Num","R","A2"]
[null,null,"USB接口数量","USBPortNum","个","Num","R","A2"]
[null,null,"以太网接口数量","EthernetPortNum ","个","Num","R","A2"]
[null,null,"光纤接口数量","FiberPortNum ","个","Num","R","A2"]
[null,null,"电压AI接口数量","AIUPortNum","个","Num","R","A2"]
[null,null,"电压AI信号","AIU","V","Num","R","A2"]
[null,null,"电流AI接口数量","AIIPortNum","个","Num","R","A2"]
[null,null,"电流AI信号","AII","A","Num","R","A2"]
[null,null,"电压AO接口数量","AOUPortNum","个","Num","R","A2"]
[null,null,"电压AO信号","AOU","V","Num","R","A2"]
[null,null,"电流AO接口数量","AOIPortNum","个","Num","R","A2"]
[null,null,"电流AO信号","AOI","A","Num","R","A2"]
[null,null,"DI干节点接口数量","DIDryNodePortNum","个","Num","R","A2"]
[null,null,"DI湿节点接口数量","DIWetNodePortNum","个","Num","R","A2"]
[null,null,"DI湿节点电压","DIWetNodeU",null,"Enum","R","D1","1. DC0～30V（标准DC24V） 2. AC110～220V 99. 其他"]
[null,null,"DO干节点接口数量","DODryNodePortNum","个","Num","R","A2"]
[null,null,"DO湿节点接口数量","DOWetNodePortNum","个","Num","R","A2"]
[null,null,"DO湿节点电压","DOWetNodeU",null,"Enum","R","D1","1. DC0～30V（标准DC24V） 2. AC110～220V 99. 其他"]
[null,null,"输入同轴线接口数量","InCoaxialPortNum","个","Num","R","A2"]
[null,null,"输出同轴线接口数量","OutCoaxialPortNum","个","Num","R","A2"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"在线状态","OnlineStatus",null,"Boolv","S","L","0. 脱线 1. 在线"]
[null,null,"上传速度","UploadSpeed","MB/s","Inst","R","L"]
[null,null,"下载速度","DownloadSpeed","MB/s","Inst","R","L"]
[null,"累计指标","累计上传数据量","AccUploadData","GB","Acc","R","L"]
[null,null,"累计下载数据量","AccDownloadData","GB","Acc","R","L"]
[null,null,"累计运行时间","AccRunTime","h","Acc","M","L"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","L"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]

{"sheet":"EGCR门禁读卡器","index":2,"n_rows":30,"n_cols":10,"rows_kept":30,"cut":false,"hidden":false,"merged":[[29,0,29,1],[28,0,28,1],[0,0,0,9],[1,0,1,1],[17,0,27,0],[17,1,23,1],[24,1,27,1],[2,0,16,1]]}
["门禁读卡器"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"门禁识别方式","RecognizeType",null,"MEnum","S","D2","1. 密码 2. 卡片 3. 纽扣钥匙 4. 指纹识别 5. 人脸识别 99. 其他 （可多选）"]
[null,null,"识别距离","RecognizeDistance","mm","Num","R","A2"]
[null,null,"识别响应时间","RecognizeResponseTime","s","Num","R","A2"]
[null,null,"有无摄像头","isCamera",null,"Bool","S","E1","0. 无 1. 有"]
[null,null,"支持卡种类","CardType",null,"Enum","M","D1","1. ID卡 2. IC卡 3. CPU卡 99. 其他"]
[null,null,"卡寿命","CardLife","年","Num","R","A2"]
[null,null,"注册卡储存容量","CardStoreCap","个","Num","R","A2"]
[null,null,"管理门数","DoorNum","组","Num","R","A2"]
[null,null,"数据传输率","DataTransferSpeed","MB/s","Num","R","A2"]
[null,null,"访问射频速率","AccessRFSpeed","MB/s","Num","R","A2"]
[null,null,"接口类型","PortType",null,"Str","M","B1"]
[null,null,"防护等级","IPGrade",null,"Str","M","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"手自动状态","ManualAutoStatus",null,"Boolv","S","L","0. 手动 1. 自动"]
[null,null,"云端控制状态","InCloudStatus",null,"Boolv","S","L","0. 非云端 1. 云端"]
[null,null,"BA手动干预状态","BAInterveneStatus",null,"Boolv","S","L","0. 不允许 1. 允许"]
[null,null,"开关状态","OpenStatus",null,"Boolv","S","L","0. 关 1. 开"]
[null,null,"记录存量","RecordStore","条","Inst","R","L"]
[null,"累计指标","累计通过人数","AccPassPersonNum","人次","Acc","R","M"]
[null,null,"累计运行时间","AccRunTime","h","Acc","S","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数",null,"设备开关设定","EquipSwitchSet",null,"Boolp","S",null,"0. 关闭 1. 开启"]
["报警消息"]

{"sheet":"EGFG速通门","index":3,"n_rows":34,"n_cols":10,"rows_kept":34,"cut":false,"hidden":false,"merged":[[32,0,32,1],[33,0,33,1],[0,0,0,9],[1,0,1,1],[21,1,27,1],[28,1,31,1],[21,0,31,0],[2,0,20,1]]}
["速通门"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"额定电压","RatedU","V","Num","R","A2"]
[null,null,"额定电流","RatedI","A","Num","R","A2"]
[null,null,"额定功率","RatedP","W","Num","R","A2"]
[null,null,"允许通行方向","AllowPassDirectionType",null,"Enum","S","D1","1. 单向 2. 双向 99. 其他"]
[null,null,"最大通行速度","MaxPassSpeed","人次/min","Num","M","A2"]
[null,null,"闸门开关时间","GateOpenTime","s","Num","R","A2"]
[null,null,"门翼摆动速度","DoorSwingSpeed","m/s","Num","R","A2"]
[null,null,"摆门长度","DoorSwingLength","m","Num","R","A2"]
[null,null,"标准通道宽度","StandardChannelWidth","m","Num","M","A2"]
[null,null,"门体材质","DoorMaterialType",null,"Enum","R","D1","1. 钢化玻璃 2. 有机玻璃 3. 亚克力板 99. 其他"]
[null,null,"提示方式","PromptMode",null,"Str","R","B1"]
[null,null,"报警方式","AlarmType",null,"MEnum","M","D2","1. 声报警 2. 光报警 99. 其他 （可多选）"]
[null,null,"支持卡种类","CardType",null,"MEnum","M","D2","1. ID卡 2. IC卡 3. CPU卡 99. 其他 （可多选）"]
[null,null,"卡寿命","CardLife","年","Num","R","A2"]
[null,null,"接口类型","PortType",null,"Str","R","B1"]
[null,null,"防护等级","IPGrade",null,"Str","M","B1","参考《11防护等级》"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange","%RH","Numr","M","A6"]
[null,null,"平均无故障时间","MTBF","h","Num","M","A2"]
["运行参数","瞬时状态","运行状态","RunStatus",null,"Boolv","S","L","0. 停止 1. 运行"]
[null,null,"故障状态","FaultStatus",null,"Boolv","S","L","0. 正常 1. 故障"]
[null,null,"手自动状态","ManualAutoStatus",null,"Boolv","S","L","0. 手动 1. 自动"]
[null,null,"云端控制状态","InCloudStatus",null,"Boolv","S","L","0. 非云端 1. 云端"]
[null,null,"BA手动干预状态","BAInterveneStatus",null,"Boolv","S","L","0. 不允许 1. 允许"]
[null,null,"通行方向","PassDirection",null,"Boolv","M","L","0. 反向 1. 正向"]
[null,null,"开关状态","OpenStatus",null,"Boolv","S","L","0. 关 1. 开"]
[null,"累计指标","累计通过人数","AccPassPersonNum","人次","Acc","R","M"]
[null,null,"累计运行时间","AccRunTime","h","Acc","S","M"]
[null,null,"开启时间计时","OpenTimeCount","h","Acc","R","M"]
[null,null,"关闭时间计时","CloseTimeCount","h","Acc","R","M"]
["设定参数"]
["报警消息"]