{"text_format":"2","workbook":"xlsx","n_sheets":4,"sheets":["PWSE强电线路","PWWE弱电线路","PWGS气体管道","PWLQ液体管道"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"PWSE强电线路","index":0,"n_rows":32,"n_cols":10,"rows_kept":32,"cut":false,"hidden":false,"merged":[[31,0,31,1],[0,0,0,9],[1,0,1,1],[27,0,29,1],[30,0,30,1],[2,0,26,1]]}
["强电线路"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"输电类型","TransType",null,"Enum","S","D1","1. 交流 1.1 低压：≤ 1kV 1.2 中压：1kV - 35kV 1.3 高压：35kV - 330kV 1.4 超高压：330kV - 1000kV 1.5 特高压：≥1000kV 2. 直流 2.1 高压直流：≤800kV 2.2 特高压直流：＞800kV 99. 其他"]
[null,null,"电气材料类型","ElecMaterialType",null,"Enum","M","D1","1. 电线 1.1 BLX型 1.2 BLV型 1.3 BX型 1.4 BV型 1.5 RV型 1.6 RX型 1.7 BVV型 1.8 RVV型 2. 电缆 2.1 VV型 2.2 YJV型 2.3 VV22型 2.4 YJV22型 2.5 ZR-YJFE型 2.6 NH-YJFE型 2.7 YJV32型 2.8 WD-ZANYJFE型 2.9 LGJ型 2.10 LGHJ型 2.11 KVV型 99. 其他"]
[null,null,"线芯导体材料","CoreMaterial",null,"Enum","M","D1","1. 铜箔丝 2. 裸铜线 3. 镀锡铜线 4. 裸绞镀铜线 5. 镀绞镀铜线 6. 镀银铜线 7. 铜包钢 8. 聚氨酯漆包线 99. 其他"]
[null,null,"导体结构","CoreStructureType",null,"Enum","R","D1","1. 硬结构 2. 软结构 99. 其他"]
[null,null,"芯数","CoreNum","根","Num","M","A2"]
[null,null,"电线长度","WireLength","m","Num","M","A2"]
[null,null,"截面积","CrossArea","mm2","Num","M","A2"]
[null,null,"传输电压","RatedU","V","Num","M","A2"]
[null,null,"最大电流","MaxI","A","Num","M","A2"]
[null,null,"输电频率","RatedFreq","Hz","Num","M","A2"]
[null,null,"20℃直流电阻率","20Resistance","Ωm","Num","R","A2"]
[null,null,"90℃直流电阻率","90Resistance","Ωm","Num","R","A2"]
[null,null,"最小弯曲半径","MinBendRadius","mm","Num","M","A2"]
[null,null,"抗拉强度","TensileStrength","MPa","Num","M","A2"]
[null,null,"绝缘材料厚度","InsulationThick","mm","Num","R","A2"]
[null,null,"绝缘材料","InsulationMaterial",null,"Enum","R","D1","1. 聚氯乙烯(PVC) 2. 聚乙烯(PE) 3. 乙烯-醋酸乙烯酯共聚物(EVA) 4. 聚丙烯(PP) 5. 聚脂料 6. 热塑性弹性体(TPE) 7. 聚氨脂(PU) 8. 热塑性聚氨脂(TPU) 99. 其他"]
[null,null,"内护套厚度","InSheathThick","mm","Num","R","A2"]
[null,null,"内保护套材料","InSheathMaterial",null,"Enum","R","D1","1. 聚氯乙烯(PVC) 2. 聚乙烯(PE) 3. 乙烯-醋酸乙烯酯共聚物(EVA) 4. 聚丙烯(PP) 5. 聚脂料 6. 热塑性弹性体(TPE) 7. 聚氨脂(PU) 8. 热塑性聚氨脂(TPU) 99. 其他"]
[null,null,"外护套厚度","OutSheathThick","mm","Num","R","A2"]
[null,null,"外保护套材料","OutSheathMaterial",null,"Enum","R","D1","1. 聚氯乙烯(PVC) 2. 聚乙烯(PE) 3. 乙烯-醋酸乙烯酯共聚物(EVA) 4. 聚丙烯(PP) 5. 聚脂料 6. 热塑性弹性体(TPE) 7. 聚氨脂(PU) 8. 热塑性聚氨脂(TPU) 99. 其他"]
[null,null,"塑胶材料特性","PlasticCharacterType",null,"Enum","R","D1","1. E 2. F 3. G 4. O 5. P 6. E-O 7. G-E 8. F-G 9. P-G 10. P-F 99. 其他","抗氧化性、耐热性、耐油性、低温柔软度、耐候性、抗臭氧性、耐磨性、电气特性、耐燃性、防潮性、抗酸性、抗碱性、抗有机溶剂（芳香族）、抗有机溶剂（脂肪族）、抗酒精性"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange","%RH","Numr","M","A6"]
[null,null,"耐火性能","FireResistanceType",null,"Enum","S","D1","1. 普通型 2. 阻燃型 3. 耐火性 4. 无卤低烟阻燃型 99. 其他"]
[null,null,"阻燃等级","FlameRetardantLev",null,"Enum","M","D1","1. HB 2. V-2 3. V-1 4. V-0 99. 其他"]
["运行参数",null,"传输电压","U","V","Inst","S","L"]
[null,null,"传输电流","I","A","Inst","S","L"]
[null,null,"输电频率","Freq","Hz","Inst","S","L"]
["设定参数"]
["报警消息"]

{"sheet":"PWWE弱电线路","index":1,"n_rows":37,"n_cols":10,"rows_kept":37,"cut":false,"hidden":false,"merged":[[36,0,36,1],[0,0,0,9],[1,0,1,1],[32,0,34,1],[35,0,35,1],[2,0,31,1]]}
["弱电线路"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数",null,"用途","UseType",null,"Enum","S","D1","1. 视频线 2. 音频线 3. 通讯电缆 4. 网线 5. 电话线 6. 信号传输线 99. 其他"]
[null,null,"线芯导体材料","CoreMaterial",null,"Enum","M","D1","1. 无氧铜 2. 纯铜 3. 镀锡铜 4. 铜包铝 5. 铝镁丝 99. 其他"]
[null,null,"有无屏蔽功能","isScreenFunc",null,"Bool","M","E1","0. 无 1. 有"]
[null,null,"传输带宽","BandWidth","MB","Num","M","A2"]
[null,null,"芯数","CoreNum","根","Num","M","A2"]
[null,null,"电线长度","WireLength","m","Num","M","A2"]
[null,null,"截面积","CrossArea","mm2","Num","M","A2"]
[null,null,"最小弯曲半径","MinBendRadius","mm","Num","M","A2"]
[null,null,"信号电压范围","SignalURange","V","Numr","M","A2"]
[null,null,"信号电流范围","SignalIRange","A","Numr","M","A2"]
[null,null,"信号频率范围","SignalFreqRange","Hz","Numr","M","A2"]
[null,null,"20℃直流电阻率","20Resistance","Ωm","Num","R","A2"]
[null,null,"90℃直流电阻率","90Resistance","Ωm","Num","R","A2"]
[null,null,"工作电容最大值","MaxElecCap","nF/m","Num","R","A2"]
[null,null,"抗拉强度","TensileStrength","MPa","Num","M","A2"]
[null,null,"绝缘材料厚度","InsulationThick","mm","Num","R","A2"]
[null,null,"绝缘材料","InsulationMaterial",null,"Enum","R","D1","1. 聚氯乙烯(PVC) 2. 聚乙烯(PE) 3. 乙烯-醋酸乙烯酯共聚物(EVA) 4. 聚丙烯(PP) 5. 聚脂料 6. 热塑性弹性体(TPE) 7. 聚氨脂(PU) 8. 热塑性聚氨脂(TPU) 99. 其他"]
[null,null,"近端串音","NearEndCrosstalk","dB(A)","Num","R","A2"]
[null,null,"近端串音功率和","NearEndCrosstalkP","W","Num","R","A2"]
[null,null,"衰减串音比","AttenuationCrosstalkRatio",null,"Num","R","A1"]
[null,null,"衰减串音比功率和","AttenuationCrosstalkRatioP","W","Num","R","A2"]
[null,null,"回波损失","ReturnLoss","dB(A)","Num","R","A2"]
[null,null,"插入损耗","InsertionLoss","dB(A)","Num","R","A2"]
[null,null,"直流环路电阻","DCLoopResistance","Ω","Num","R","A2"]
[null,null,"传播时延","PropagateDelay","μs","Num","R","A2"]
[null,null,"传播时延偏差","PropagateDelayDeviation","μs","Num","R","A2"]
[null,null,"工作温度范围","WorkTempRange","℃","Numr","M","A6"]
[null,null,"工作湿度范围","WorkRHRange","%RH","Numr","M","A6"]
[null,null,"耐火性能","FireResistanceType",null,"Enum","S","D1","1. 普通型 2. 阻燃型 3. 耐火性 4. 无卤低烟阻燃型 99. 其他"]
[null,null,"阻燃等级","FlameRetardantLev",null,"Enum","M","D1","1. HB 2. V-2 3. V-1 4. V-0 99. 其他"]
["运行参数",null,"信号电压","U","V","Inst","S","L"]
[null,null,"信号电流","I","A","Inst","S","L"]
[null,null,"信号频率","Freq","Hz","Inst","S","L"]
["设定参数"]
["报警消息"]

{"sheet":"PWGS气体管道","index":2,"n_rows":55,"n_cols":10,"rows_kept":55,"cut":false,"hidden":false,"merged":[[53,0,53,1],[54,0,54,1],[31,1,35,1],[0,0,0,9],[1,0,1,1],[46,0,52,1],[36,1,39,1],[40,1,42,1],[43,1,45,1],[2,0,45,0],[2,1,30,1]]}
["气体管道"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数","整体","用途","UseType",null,"Enum","S","D1","1. 普通空调系统用风管(PK) 1.1 送风 1.2 回风 1.3 排风 1.4 新风 1.5 加压送风 1.6 厨房排油烟 2. 防排烟系统用风管(PY) 2.1 消防补风 2.2 排烟 3. 含酸碱排风系统用风管(PF) 4. 燃气系统送燃气 5. 气体灭火剂管 99. 其他"]
[null,null,"材质种类","MaterialType",null,"Enum","M","D1","1. 镀锌钢板 2. 无机玻璃钢 3. 纤维织物 4. 复合玻纤板 99. 其他"]
[null,null,"截面形状","CrossShapeType",null,"Enum","S","D1","1. 圆形 2. 矩形 3. 扁圆形 99. 其他"]
[null,null,"管段类型","PipeType",null,"Enum","M","D1","1. 直管 2. 弯管 3. 三通 4. 四通 5. 变径 99. 其他"]
[null,null,"管段长度","PipeLength","m","Num","M","A2"]
[null,null,"尺寸稳定性","SizeStability","%","Num","R","A2"]
[null,null,"是否密封","IsSeal",null,"Bool","M","E1","0. 否 1. 是"]
[null,null,"渗透率","Permeability","%","Num","M","A2"]
[null,null,"沿程比摩阻","SpecificFrictionalResistance","Pa/m","Num","M","A2"]
[null,null,"允许漏风量","AllowAirLeakFlow","m3/h","Num","M","A2"]
[null,null,"导热系数","HeatConductCoeff","W/(mK)","Num","R","A2"]
[null,null,"弯曲强度","BendStrength","MPa","Num","R","A2"]
[null,null,"压缩强度","CompressStrength","MPa","Num","R","A2"]
[null,null,"压力等级","PressLev",null,"Enum","M","D1","1. 低压L 2. 中压M 3. 高压H 4. 超高压U 99. 其他"]
[null,null,"耐火性能","FireResistanceType",null,"Bool","M","E1","0. 普通风管（P) 1. 耐火风管（N）"]
[null,null,"风管释放有害气体浓度","HarmfulGas","mg/m2","Num","R","A2"]
[null,null,"吸水率","WaterAbsorption","%","Num","R","A2",null,"表示物体在正常大气压下吸水程度"]
[null,null,"断裂伸长率","BreakElongation","%","Num","R","A2",null,"指试样在拉断时的位移值与原长的比值"]
[null,null,"噪声限值","NoiseLimit","dB(A)","Num","R","A2"]
[null,null,"噪声系数","NoiseCoeff",null,"Num","R","A1"]
[null,null,"连接形式","ConnectType",null,"Enum","M","D1","1. 金属矩形风管 1.1 角钢法兰 1.2 薄钢板法兰 1.3 S型插条 1.4 C型插条 1.5 立联合角型插条 1.6 立咬口 2. 金属圆形风管 2.1 角钢法兰连接 2.2 承插连接 2.3 芯管连接 2.4 立筋抱箍连接 2.5 抱箍连接 3. 非金属矩形连接3.1 45度粘接 3.2 榫接 3.3 槽形插接连接 3.4 工形插接连接 3.5 外套角钢法兰 3.6 C形插接法兰 3.7 外套槽形法兰 3.8 H连接法兰 99. 其他"]
[null,null,"设计进口风速","DesignInV","m/s","Num","M","A2"]
[null,null,"设计出口风速","DesignOutV","m/s","Num","M","A2"]
[null,null,"设计进口压力","DesignInPress","Pa","Num","M","A2"]
[null,null,"设计出口压力","DesignOutPress","Pa","Num","M","A2"]
[null,null,"设计风量","DesignFlow","m3/h","Num","M","A2"]
[null,null,"设计输送气体密度","DesignGasDensity","kg/m3","Num","M","A2"]
[null,null,"设计输送气体温度","DesignGasTemp","℃","Num","M","A2"]
[null,null,"设计输送气体相对湿度","DesignGasRH","%RH","Num","M","A2"]
[null,"保温材料","是否有保温层","IsInsulation",null,"Bool","S","E1","0. 无 1. 有"]
[null,null,"保温材料厚度","InsulationThick","mm","Num","M","A2"]
[null,null,"保温材料种类","InsulationMatierial",null,"Enum","M","D1","1. 岩棉 2. 离心玻璃棉 3. 橡塑海绵 4. 阻燃聚乙烯泡沫塑料 5. 硬质聚氨酯泡沫塑料 99. 其他"]
[null,null,"保温材料密度","InsulationDensity","kg/m3","Num","R","A2"]
[null,null,"保温材料导热系数","InsulationHeatConductCoeff","W/(mK)","Num","R","A2"]
[null,"矩形风管","宽","RectangleWidth","mm","Num","S","A2"]
[null,null,"高","RectangleHeight","mm","Num","S","A2"]
[null,null,"弯管曲率","RectangleBendCurvature",null,"Num","R","A1"]
[null,null,"弯管平面边长","RectangleBendFlatSideLength","mm","Num","R","A2"]
[null,"圆形风管","公称直径","CircularNorminalDiameter","mm","Num","S","A2"]
[null,null,"曲率半径","CircularCurvatureRadius","mm","Num","R","A2"]
[null,null,"弯管角度","CircularBendAngle","°","Num","R","A2"]
[null,"扁圆形风管","长轴","OblatenessLongAxis","mm","Num","M","A2"]
[null,null,"短轴","OblatenessShortAxis","mm","Num","M","A2"]
[null,null,"弯管角度","OblatenessBendAngle","°","Num","R","A2"]
["运行参数",null,"进口风速","InV","m/s","Inst","S","L"]
[null,null,"出口风速","OutV","m/s","Inst","R","L"]
[null,null,"进口温度","InTemp","℃","Inst","S","L"]
[null,null,"出口温度","OutTemp","℃","Inst","R","L"]
[null,null,"进口压力","InPress","Pa","Inst","S","L"]
[null,null,"出口压力","OutPress","Pa","Inst","R","L"]
[null,null,"瞬时风量","Flow","m3/h","Inst","S","L"]
["设定参数"]
["报警消息"]

{"sheet":"PWLQ液体管道","index":3,"n_rows":39,"n_cols":10,"rows_kept":39,"cut":false,"hidden":false,"merged":[[37,0,37,1],[38,0,38,1],[30,0,36,1],[22,1,26,1],[0,0,0,9],[1,0,1,1],[2,0,29,0],[2,1,21,1],[27,1,29,1]]}
["液体管道"]
["分级标签",null,"信息点","信息点编码","单位","类型","优先级","输入方式","字典选择"," 备注"]
["技术参数","整体","用途","UseType",null,"Enum","S","D1","1. 给排水系统 1.1 生活给水 1.2 生活热水给水 1.3 直饮水给水 1.4 中水给水 1.5 其他公共给水（水景、喷灌、泳池等） 1.6 污水排水 1.7 雨水收集 2. 空调系统 2.1 冷冻水 2.2 冷却水 2.3 采暖热水 2.4 采暖蒸汽 2.5 制冷剂 2.6 吸收剂 2.7 乙二醇 3. 消防系统 3.1 消防给水 3.2 液体灭火剂 4. 特殊 4.1 燃油 4.2 液化天然气 99. 其他"]
[null,null,"材质种类","MaterialType",null,"Enum","M","D1","1. 不锈钢类 1.1 304材料 1.2 316材料 2. 碳钢类 2.1 热镀锌 2.2 冷镀锌 3. 铜管类 3.1 全铜 3.2 黄铜 4. 复合管类 4.1 钢塑复合 4.2 铝塑复合 4.3 铜塑复合 4.4 不锈钢复合 5. 塑料管类 5.1 PP-R 5.2 ABS 5.3 PE 5.4 PVC 99. 其他"]
[null,null,"管段类型","PipeType",null,"Enum","M","D1","1. 直管 2. 弯管 3. 三通 4. 四通 5. 变径 99. 其他"]
[null,null,"管段长度","PipeLength","m","Num","M","A2"]
[null,null,"公称直径","NominalDiameter","mm","Num","S","A2"]
[null,null,"壁厚","WallThick","mm","Num","S","A2"]
[null,null,"标准尺寸比","StandardSizeRatio",null,"Num","R","A1",null,"标准尺寸比是管的公称外径与公称壁厚之间的比值"]
[null,null,"沿程比摩阻","SpecificFrictionalResistance","Pa/m","Num","M","A2"]
[null,null,"设计进口流速","DesignInV","m/s","Num","M","A2"]
[null,null,"设计出口流速","DesignOutV","m/s","Num","M","A2"]
[null,null,"设计流量","DesignFlow","m3/h","Num","M","A2"]
[null,null,"设计进口压力","DesignInPress","MPa","Num","M","A2"]
[null,null,"设计出口压力","DesignOutPress","MPa","Num","M","A2"]
[null,null,"设计输送液体温度","DesignLiquidTemp","℃","Num","M","A2"]
[null,null,"设计输送液体PH值","DesignLiquidPH",null,"Num","M","A1"]
[null,null,"设计输送液体密度","DesignLiquidDensity","kg/m3","Num","M","A2"]
[null,null,"管道级别","PipeLev",null,"Enum","M","D1","1. Ⅰ 2. Ⅱ 3. Ⅲ 4. Ⅳ 99. 其他","Ⅰ:操作压力>6.4Mpa，操作温度>450℃；-140~-45℃\nⅡ:操作压力>4~6.4Mpa，操作温度>350~450℃；> -45~ -30℃\nⅢ:操作压力>1.6~4Mpa，操作温度>200~350℃；> -30~ -20℃\nⅣ:操作压力≤1.6Mpa，操作温度> -20~ 200℃"]
[null,null,"压力等级","PressLev",null,"Enum","M","D1","1. 低压L 2. 中压M 3. 高压H 4. 超高压U 99. 其他"]
[null,null,"最小屈服强度","MinYieldStrength","MPa","Num","M","A2"]
[null,null,"强度设计系数","StrengthDesignCoeff",null,"Num","R","A1"]
[null,"保温材料","是否有保温层","IsInsulation",null,"Bool","S","E1","0. 无 1. 有"]
[null,null,"保温材料厚度","InsulationThick","mm","Num","M","A2"]
[null,null,"保温材料种类","InsulationMatierial",null,"Enum","M","D1","1. 岩棉 2. 离心玻璃棉 3. 橡塑海绵 4. 阻燃聚乙烯泡沫塑料 5. 硬质聚氨酯泡沫塑料 99. 其他"]
[null,null,"保温材料密度","InsulationDensity","kg/m3","Num","R","A2"]
[null,null,"保温材料导热系数","InsulationHeatConductCoeff","W/(mK)","Num","R","A2"]
[null,"塑料管","材料分级","PlasticMaterialLev",null,"Enum","M","D1","1. 1级 2. 2级 3. 3级 4. 4级 5. 5级 6. 6级 7. 7级 99. 其他"]
[null,null,"炭黑含量","PlasticCarbonBlackContent","%","Num","R","A2"]
[null,null,"挥发分含量","PlasticVolatileContent","%","Num","R","A2"]
["运行参数",null,"进口流速","InV","m/s","Inst","S","L"]
[null,null,"出口流速","OutV","m/s","Inst","R","L"]
[null,null,"进口温度","InTemp","℃","Inst","S","L"]
[null,null,"出口温度","OutTemp","℃","Inst","R","L"]
[null,null,"进口压力","InPress","MPa","Inst","S","L"]
[null,null,"出口压力","OutPress","MPa","Inst","R","L"]
[null,null,"瞬时流量","Flow","m3/h","Inst","S","L"]
["设定参数"]
["报警消息"]