{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":192,"n_cols":8,"rows_kept":192,"cut":false,"hidden":false,"merged":[[0,7,1,7],[0,6,1,6],[2,0,20,0],[2,1,20,1],[2,2,6,2],[2,3,6,3],[7,2,8,2],[7,3,8,3],[9,2,10,2],[9,3,10,3],[13,2,15,2],[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,5,1,5],[21,0,40,0],[21,1,40,1],[21,2,22,2],[21,3,22,3],[24,2,28,2],[13,3,15,3],[16,2,17,2],[16,3,17,3],[18,2,19,2],[18,3,19,3],[74,2,81,2],[74,3,81,3],[82,2,88,2],[82,3,88,3],[24,3,28,3],[29,2,30,2],[29,3,30,3],[31,2,37,2],[31,3,37,3],[38,2,40,2],[38,3,40,3],[89,2,92,2],[89,3,92,3],[93,2,95,2],[93,3,95,3],[96,0,135,0],[96,1,135,1],[96,2,99,2],[96,3,99,3],[100,2,111,2],[100,3,111,3],[41,0,95,0],[41,1,95,1],[41,2,59,2],[41,3,59,3],[60,2,73,2],[60,3,73,3],[112,2,115,2],[112,3,115,3],[116,2,117,2],[116,3,117,3],[118,2,121,2],[118,3,121,3],[122,2,124,2],[122,3,124,3],[125,2,128,2],[125,3,128,3],[130,2,131,2],[130,3,131,3],[132,2,134,2],[132,3,134,3],[136,0,178,0],[136,1,178,1],[136,2,140,2],[136,3,140,3],[141,2,143,2],[141,3,143,3],[144,2,147,2],[144,3,147,3],[148,2,150,2],[148,3,150,3],[151,2,166,2],[151,3,166,3],[167,2,170,2],[167,3,170,3],[190,2,191,2],[190,3,191,3],[172,2,177,2],[172,3,177,3],[179,0,191,0],[179,1,191,1],[179,2,183,2],[179,3,183,3],[184,2,186,2],[184,3,186,3],[187,2,189,2],[187,3,189,3]]}
["专业编码","专业名称（非实体）","系统类型编码","系统类型名称","设备类型编码","设备类型名称","粗略对应分项标签","租户标签"]
[]
["1","强电专业","1","变配电系统","1","变压器"]
[{"$nulls":4},"2","高压开关柜"]
[{"$nulls":4},"3","变配电低压开关柜"]
[{"$nulls":4},"4","直流屏"]
[{"$nulls":4},"5","变配电母线插接箱"]
[null,null,"2","柴发机房系统","1","柴油发电机"]
[{"$nulls":4},"2","柴发低压开关柜"]
[null,null,"3","备用电源系统","1","备用电源"]
[{"$nulls":4},"2","备用电源低压开关柜"]
[null,null,"4","机房动力系统","1","机房动力低压开关柜"]
[null,null,"5","室外动力系统","1","室外动力低压开关柜"]
[null,null,"6","电梯系统","1","直梯"]
[{"$nulls":4},"2","扶梯"]
[{"$nulls":4},"3","电梯低压开关柜"]
[null,null,"7","照明系统","1","照明灯具"]
[{"$nulls":4},"2","照明低压开关柜"]
[null,null,"8","租户配电系统","1","租户低压开关柜"]
[{"$nulls":4},"2","租户母线插接箱"]
[null,null,"9","强电人防系统","1","人防低压开关柜"]
["2","弱电专业","1","楼宇自控系统","1","楼控主机"]
[{"$nulls":4},"2","楼控网络控制器"]
[null,null,"2","电视信号系统","1","电视前端设备"]
[null,null,"3","多媒体信息发布系统","1","多媒体主机"]
[{"$nulls":4},"2","播放器"]
[{"$nulls":4},"3","LED大屏"]
[{"$nulls":4},"4","多媒体显示屏"]
[{"$nulls":4},"5","自助终端机"]
[null,null,"4","无线对讲系统","1","对讲机"]
[{"$nulls":4},"2","中继台"]
[null,null,"5","车库管理系统","1","车库主机"]
[{"$nulls":4},"2","车库网络控制器"]
[{"$nulls":4},"3","车库摄像头"]
[{"$nulls":4},"5","车库显示屏"]
[{"$nulls":4},"4","进出闸机"]
[{"$nulls":4},"6","机械车位"]
[{"$nulls":4},"7","充电桩"]
[null,null,"6","本地网络系统","1","路由器"]
[{"$nulls":4},"2","交换机"]
[{"$nulls":4},"3","硬件防火墙"]
["3","空调专业","1","中央供冷系统","1","离心机",121111]
[{"$nulls":4},"2","螺杆机",121111]
[{"$nulls":4},"3","吸收机",121111]
[{"$nulls":4},"4","空气源热泵",121122,121111]
[{"$nulls":4},"5","水源热泵",121122,121111]
[{"$nulls":4},"6","地源热泵",121122,121111]
[{"$nulls":4},"7","冷却塔",121114]
[{"$nulls":4},"8","供冷冷冻水泵",121112]
[{"$nulls":4},"9","供冷冷却水泵",121113]
[{"$nulls":4},"A","供冷乙二醇泵",12111]
[{"$nulls":4},"B","供冷补水泵",12111]
[{"$nulls":4},"C","供冷定压补水装置",12111]
[{"$nulls":4},"D","供冷板式换热器",12111]
[{"$nulls":4},"E","供冷容积式换热器",12111]
[{"$nulls":4},"F","供冷真空脱气机",12111]
[{"$nulls":4},"G","供冷水加药装置",12111]
[{"$nulls":4},"H","供冷软化水装置",12111]
[{"$nulls":4},"I","供冷全程水处理仪",12111]
[{"$nulls":4},"J","蓄冰槽",12111]
[null,null,"2","中央供热系统","1","供热燃煤锅炉",101]
[{"$nulls":4},"2","供热燃油锅炉",61]
[{"$nulls":4},"3","供热燃气锅炉",51]
[{"$nulls":4},"4","供热电锅炉",121121]
[{"$nulls":4},"5","供热水泵",121123]
[{"$nulls":4},"6","供热补水泵",12112]
[{"$nulls":4},"7","供热定压补水装置",12112]
[{"$nulls":4},"8","供热板式换热器",12112]
[{"$nulls":4},"9","供热容积式换热器",12112]
[{"$nulls":4},"A","供热真空脱气机",12112]
[{"$nulls":4},"B","供热水加药装置",12112]
[{"$nulls":4},"C","供热软化水装置",12112]
[{"$nulls":4},"D","供热全程水处理仪",12112]
[{"$nulls":4},"E","地板采暖设备",12112]
[null,null,"3","空调末端系统","1","空调机组",12121]
[{"$nulls":4},"2","新风机组",12122]
[{"$nulls":4},"3","风机盘管",12123]
[{"$nulls":4},"4","分体空调",12124]
[{"$nulls":4},"5","变频多联机",12125]
[{"$nulls":4},"6","VAVBOX",12123]
[{"$nulls":4},"7","地板空调器",1212]
[{"$nulls":4},"8","空调风口",1212]
[null,null,"4","通风系统","1","通风送风机",1231]
[{"$nulls":4},"2","通风排风机",1231]
[{"$nulls":4},"3","通风诱导风机",1231]
[{"$nulls":4},"4","热风幕",12126]
[{"$nulls":4},"5","空气净化器",1231]
[{"$nulls":4},"6","除味装置",1231]
[{"$nulls":4},"7","通风风口",1231]
[null,null,"5","厨房排油烟系统","1","厨房送风机",12313]
[{"$nulls":4},"2","厨房排风机",12313]
[{"$nulls":4},"3","油烟净化器",1231]
[{"$nulls":4},"4","厨房风口",1231]
[null,null,"6","空调人防系统","1","人防排风机",1231]
[{"$nulls":4},"2","滤毒除湿机",1231]
[{"$nulls":4},"3","人防风口",1231]
["4","给排水专业","1","生活给水系统","1","生活给水供水机组",1232]
[{"$nulls":4},"2","生活给水水箱消毒器",1232]
[{"$nulls":4},"3","生活给水紫外线消毒器",1232]
[{"$nulls":4},"4","生活给水储水箱",1232]
[null,null,"2","生活热水系统","1","热水燃煤锅炉",101]
[{"$nulls":4},"2","热水燃油锅炉",61]
[{"$nulls":4},"3","热水燃气锅炉",52]
[{"$nulls":4},"4","热水电锅炉",121121]
[{"$nulls":4},"5","燃气热水器",12112]
[{"$nulls":4},"6","电热水器",12112]
[{"$nulls":4},"7","太阳能集热器",12112]
[{"$nulls":4},"8","辅热设备",12112]
[{"$nulls":4},"9","热水板式换热器",12112]
[{"$nulls":4},"A","热水容积式换热器",12112]
[{"$nulls":4},"B","热水水泵",12112]
[{"$nulls":4},"C","热水储水箱",12112]
[null,null,"3","中水系统","1","中水给水供水机组",1232]
[{"$nulls":4},"2","中水处理机组",1232]
[{"$nulls":4},"3","中水储水箱",1232]
[{"$nulls":4},"4","雨水收集设备",1232]
[null,null,"4","直饮水系统","1","直饮水处理机组",1232]
[{"$nulls":4},"2","即时加热器",1232]
[null,null,"5","污水处理系统","1","污废水一体式提升机组",1232]
[{"$nulls":4},"2","潜污泵",1232]
[{"$nulls":4},"3","餐饮除油成套设备",1232]
[{"$nulls":4},"4","化粪池",1232]
[null,null,"6","喷灌系统","1","喷灌机组",1232]
[{"$nulls":4},"2","喷灌喷头",1232]
[{"$nulls":4},"3","喷灌控制器",1232]
[null,null,"7","水景系统","1","水景循环过滤机组",1232]
[{"$nulls":4},"2","水景喷头",1232]
[{"$nulls":4},"3","水景控制器",1232]
[{"$nulls":4},"4","水景灯具",1232]
[null,null,"8","泳池系统","1","泳池循环过滤机组",1232]
[null,null,"9","燃气系统","1","燃气调压箱",5]
[{"$nulls":4},"2","液化石油气瓶",5]
[null,null,"A","给排水电伴热系统","1","给排水伴热电缆",1232]
[{"$nulls":4},"2","给排水伴热保温器",1232]
[{"$nulls":4},"3","给排水伴热控制器",1232]
[null,null,"B","给排水人防系统","1","人防储水箱",1232]
["5","消防专业","1","火灾报警系统","1","火灾报警主机",1413]
[{"$nulls":4},"2","火灾报警显示屏",1413]
[{"$nulls":4},"3","联动琴台",1413]
[{"$nulls":4},"4","火灾探测器",1413]
[{"$nulls":4},"5","声光报警器",1413]
[null,null,"2","燃气报警系统","1","燃气报警主机",1413]
[{"$nulls":4},"2","燃气探测器",1413]
[{"$nulls":4},"3","燃气切断阀",1413]
[null,null,"3","漏电火灾报警系统","1","漏电火灾报警主机",1413]
[{"$nulls":4},"2","漏电探测器",1413]
[{"$nulls":4},"3","电流探测器",1413]
[{"$nulls":4},"4","温度探测器",1413]
[null,null,"4","紧急广播及背景音乐系统","1","广播前端设备",1413]
[{"$nulls":4},"2","广播分区控制器",1413]
[{"$nulls":4},"3","扬声器",1413]
[null,null,"5","消防给水系统","1","消火栓供水加压泵",1413]
[{"$nulls":4},"2","喷淋供水加压泵",1413]
[{"$nulls":4},"3","水喷雾供水加压泵",1413]
[{"$nulls":4},"4","停机坪消防供水加压泵",1413]
[{"$nulls":4},"5","消防水炮设备",1413]
[{"$nulls":4},"6","消防稳压设备",1413]
[{"$nulls":4},"7","泡沫储罐组",1413]
[{"$nulls":4},"8","空压机",1413]
[{"$nulls":4},"9","湿式报警阀组",1413]
[{"$nulls":4},"A","干式报警阀组",1413]
[{"$nulls":4},"B","预作用报警阀组",1413]
[{"$nulls":4},"C","消火栓箱",1413]
[{"$nulls":4},"D","室外消火栓",1413]
[{"$nulls":4},"E","水泵接合器",1413]
[{"$nulls":4},"F","消防伴热电缆",1413]
[{"$nulls":4},"G","末端试水装置",1413]
[null,null,"6","气体灭火系统","1","气体灭火瓶组",1413]
[{"$nulls":4},"2","气体灭火启动瓶",1413]
[{"$nulls":4},"3","气体灭火控制器",1413]
[{"$nulls":4},"4","气体灭火喷头",1413]
[null,null,"7","灭火器系统","1","灭火器",1413]
[null,null,"8","防排烟系统","1","排烟风机",1413]
[{"$nulls":4},"3","排烟补风机",1413]
[{"$nulls":4},"4","事故排风机",1413]
[{"$nulls":4},"5","排烟风口",1413]
[{"$nulls":4},"7","排烟阀",1413]
[{"$nulls":4},"8","防火阀",1413]
[null,null,"9","防火卷帘门系统","1","防火卷帘门",1413]
["6","安防专业","1","视频监控系统","1","监控主机",1414]
[{"$nulls":4},"2","监控摄像头",1414]
[{"$nulls":4},"3","监控前端设备",1414]
[{"$nulls":4},"4","监视器",1414]
[{"$nulls":4},"5","硬盘录像机",1414]
[null,null,"2","巡更系统","1","巡更主机",1414]
[{"$nulls":4},"2","巡更通讯座",1414]
[{"$nulls":4},"3","巡更棒",1414]
[null,null,"3","门禁系统","1","门禁控制器",1414]
[{"$nulls":4},"2","门禁读卡器",1414]
[{"$nulls":4},"3","速通门",1414]
[null,null,"4","入侵报警系统","1","入侵报警主机",1414]
[{"$nulls":4},"2","入侵报警探测器",1414]